{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Graph2","Graph2 (2)","strobridge","Graph1","T°barycentre"],"not_rendered":{"charts":6,"images":0,"macros":0,"external_links":3,"defined_names":27,"comments":1,"pivot_tables":0},"unopened":[{"sheet":"Graph2","index":0,"reason":"not_a_worksheet"},{"sheet":"Graph2 (2)","index":1,"reason":"not_a_worksheet"},{"sheet":"Graph1","index":3,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"strobridge","index":2,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Cycles","Puissance à 4,5K en kW","Rdt Carnot avec P compresseur idéale"]
["KSTAR",9.6,0.434]
["ITER Isabelle",26.9,0.443]
["LEP 6 kW AL",6.3,0.45900000000000002]
["LEP 6 kW LINDE",6.1,0.53500000000000003]
["LEP 12 kW AL",12.1,0.58499999999999996]
["LEP 12 kW LINDE",11.9,0.57599999999999996]
["LEP 18 kW",19.5,0.45500000000000002]
["LHC 18 kW AL",17.899999999999999,0.50900000000000001]
["LHC 18 kW LINDE",18.3,0.49]
["JT 60 3T",10.6,0.437]
["JT 60 6T",10.7,0.46200000000000002]
["QATAR",9,0.28399999999999997]
["RHEA",21.8,0.33]
["SKIKDA",9.1999999999999993,0.28799999999999998]
["ITER PH4 max",36.700000000000003,0.58399999999999996]
["ITER PH4 min",12.8,0.38100000000000001]
["ESS OLD",9.1999999999999993,0.51259999999999994]
["ESS NEW",10.35,0.51400000000000001]

{"sheet":"T°barycentre","index":4,"n_rows":22,"n_cols":6,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Cycles","Rdt cycle en W/W@4,5K (compresseurs isoT)","T° barycentre","rdt Carnot","remarque"]
[null,"QATAR",231,70.099999999999994,0.28399999999999997]
[null,"Rhéa",210,70.099999999999994,0.33]
[null,"SKIKDA",235,68.5,0.28799999999999998,"avec puissance N2à 5W/W"]
[null,"JT 60 3T","119 (avec N2 à 1W/W) / 154 (avec N2 à 5W/W)",36.1,0.437,"avec puissance N2à 5W/W"]
[null,"JT 60 6T",141,35.299999999999997,0.46200000000000002]
[null,"KSTAR",156,28,0.434]
[null,"LHC 18 kW LINDE",134,24.8,0.49399999999999999]
[null,"LHC 18 kW AL",129,24.5,0.50900000000000001]
[null,"ITER (mean power) Isabelle","120 (avec N2 à 1W/W) / 155 (avec N2 à 8W/W)",23.7,0.443,"avec puissance N2à 8W/W"]
[null,"ITER (maxi power) Isabelle","118 (avec N2 à 1W/W) / 146,5 (avec N2 à 8W/W)",18.21,0.44800000000000001,"avec puissance N2à 8W/W"]
[null,"ITER (min power) Isabelle","127 (avec N2 à 1W/W) / 171 (avec N2 à 8W/W)",29.07,0.38500000000000001,"avec puissance N2à 8W/W"]
[null,"LEP 18 kW",142,19.8,0.41699999999999998]
[null,"LEP 6 kW LINDE",126,15.3,0.53500000000000003]
[null,"LEP 6 kW AL",143,14.7,0.45900000000000002]
[null,"LEP 12 kW LINDE",116,13.4,0.57599999999999996]
[null,"LEP 12 kW AL",115,13.6,0.58499999999999996]
[null,"ITER PH4 max",224,8.8000000000000007,0.58399999999999996]
[null,"ITER PH4 min",524,14.4,0.38100000000000001]
[null,"ESS OLD",137.5,15.497,{"$f":"strobridge!C18","v":0.51259999999999994}]
[null,"ESS NEW",null,13.99,0.51400000000000001]