{"text_format":"1","workbook":"xlsx","n_sheets":28,"sheets":["Main","ExergyBalance","Exergy_Graph","TS Setup","TS_Graph","LNG","CoolerHeater","Compressors","Turbines","ExergyData","TSAuxData","DS_HX_Template","Streams Summary","AUX","DS-HX-01","DS-HX-02","DS-HX-03","DS-HX-04","DS-HX-05","DS-HX-06","DS-HX-07","DS-HX-08","DS-HX-09","DS-HX-10","DS-HX-11","DS-HX-12","DS-HX-13","DS-HX-VLP"],"not_rendered":{"charts":4,"images":15,"macros":1,"external_links":0,"defined_names":104,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Exergy_Graph","index":2,"reason":"not_a_worksheet"},{"sheet":"TS_Graph","index":4,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":46,"n_cols":32,"rows_kept":46,"cut":false,"hidden":false,"merged":[[2,9,2,10],[2,12,2,13],[2,14,2,15],[21,1,21,6],[29,0,29,2]]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPLETE"]
[null,null,null,null,null,null,{"$f":"J3","v":"Exergy Investment"},{"$f":"SUM(K4:K52)","v":-1567674.484828484},null,"Exergy Investment",null,"Energy Invest.","Exergy Use",null,"Exergy Loss",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WCS LP/MP",-539968.64368309919,-1456043.3789961054]
[null,null,null,null,null,null,{"$f":"M3","v":"Exergy Use"},{"$f":"SUM(N4:N52)","v":712738.62873993046},null,"C-LP/MP",-602486.18130932003,-1255179.5443944167,"2K Loops",574295.33905139146,"Adsobers",2776.1900051769335,null,null,null,null,null,null,null,null,null,null,null,null,null,"WCS MP/HP",-810352.81632012501]
["Reference warm temperature for exergy",null,null,300,null,null,{"$f":"O3","v":"Exergy Loss"},{"$f":"SUM(P4:P52)","v":854935.85608855227},null,"C-MP/HP",-866541.87224991433,-1805295.5671873216,"TS",79925.64318135893,"ORS",15474.288842745125,null,null,null,null,null,null,null,null,null,null,null,null,null,"WCS VLP/LP",-94751.296745192958]
["Reference cold temperature for exergy",null,null,4.5,null,null,"Exergy Balance",{"$f":"H3+H4+H5","v":-1.280568540096283E-9},null,"C-VLP/LP",-87675.809021561407,-182657.93546158628,"RF Coupler",58517.646507180099,"Dewar w Heat Loss",16848.089336009318,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cold compressors",-10970.622247688239]
[null,null,null,null,null,null,"Relative difference",{"$f":"1-ABS((H5+H4)/H3)","v":0},null,"Electricity CC-100",-2361.4692932041776,-2361.4692932041776,null,null,"WCS Bypass",0,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nitrogen"]
["Specific W/W",{"$f":"(_TRef-_TRefCold)/_TRefCold","v":65.666666666666671},null,null,null,null,null,null,null,"Electricity CC-101",-4224.9887737807958,-4224.9887737807958,null,null,"VLV-HP/LP",54366.353699490137]
["Carnot efficiency",{"$f":"1/_WpW","v":1.5228426395939085E-2},null,null,null,null,null,null,null,"Electricity CC-102",-4384.1641807032656,-4384.1641807032656,null,null,"JT Valve",6477.2511054970091,null,null,null,null,null,null,null,null,null,null,null,null,null,"Comp bypass",50841.149206687405,1456043.3789960998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-01",27456.970239330083,null,null,null,null,null,null,null,null,null,null,null,null,null,"ORS",14470.910303638317]
[null,null,null,"Group all elements",null,null,null,null,null,null,null,null,null,null,"HX-02",5654.2239399459213,null,null,null,null,null,null,null,null,null,null,null,null,null,"Piping",15786.208202941576]
["Heat exchanger",null,null,"NO",null,null,null,null,null,null,null,null,null,null,"HX-03",32657.416357344016,null,null,null,null,null,null,null,null,null,null,null,null,null,"Adsorbers",3032.4633045860101]
["Compressor",null,null,"NO",null,null,null,null,null,null,null,null,null,null,"HX-04",9419.2320972122252,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cold compressors",88290.464342758656]
["Valves",null,null,"NO",null,null,{"$f":"\"Useful power @ \" & _TRefCold&\" K\"","v":"Useful power @ 4.5 K"},null,null,null,null,null,null,null,"HX-05",880.02648664452136,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-01",42895.289712170139]
["Mixer",null,null,"YES",null,null,{"$f":"_ExUse/_WpW","v":10853.887747308585},null,null,null,null,null,null,null,"HX-06",9520.5106717431918,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-02",9169.0201220847666]
["Piping",null,null,"YES",null,null,"Ideal cycle efficiency","Real cycle efficiency",null,null,null,null,null,null,"HX-07",1008.6062102401629,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-03",30415.298838967457]
["Turbines",null,null,"NO",null,null,{"$f":"-_ExInv/_UsefulPower","v":144.43437423767506},{"$f":"-SUM(L4:L52)/_UsefulPower","v":299.80996165156819},null,null,null,null,null,null,"HX-08",19572.098373377696,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-04",8614.4701670836657]
["Add bearing losses to turbine",null,null,"NO",null,null,"Ideal Carnot efficiency","Real Carnot efficiency",null,null,null,null,null,null,"HX-09",13824.346452806611,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-05",972.97750709298998]
["Add inlet Dp to turbine",null,null,"NO",null,null,{"$f":"-_ExUse/_ExInv","v":0.45464708116233055},{"$f":"_WpW/_Eff_WW_Real","v":0.21902763438855599},null,null,null,null,null,null,"HX-10",15662.969471445773,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-06",11304.539735231549]
["Group bearing & inlet Dp if separated",null,null,"NO",null,null,null,null,null,null,null,null,null,null,"HX-11",18310.295193345053,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-07",2605.8572598686442]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-12",6402.9448964056792,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-08",25647.19119626563]
["Root Path","D:\\USERS\\GOLO.ZICK\\DESKTOP\\ESS\\FINAL\\",null,null,null,null,null,null,null,null,null,null,null,null,"HX-13",1812.7421743749292,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-09",10271.093213312328]
["Hysys case","ST!SC_MML__HX-VLP.HSC",null,null,null,null,null,null,null,null,null,null,null,null,"HX-VLP",68596.128651737003,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-10",7961.9525935440324]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bearing Feed gas",51396.391007351485,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-11",13577.757743562572]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turbine bearing losses",10310.582256305939,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-12",6399.0247347590048]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turbine inlet Dp losses",11829.715977417072,null,null,null,null,null,null,null,null,null,null,null,null,null,"HX-13",1810.2867463351868]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-1",33019.837760486058,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-1",37948.686111236806]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-2",37375.987571531907,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-2",27540.22172119841]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-3",61244.283271490014,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-3",63336.216672444483]
["Stream Summary units",null,null,null,null,null,"Total # of turbines",null,null,null,null,null,null,null,"T-4",91097.04065854731,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-4",80371.277643780806]
["Temperature",null,"K",null,null,null,{"$f":"COUNTA(Turbines!A2:A1048576)","v":6},null,null,null,null,null,null,null,"T-5",79863.16003873467,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-5",77626.72257123678]
["Pressure",null,"bar",null,null,null,"Total turbine power",null,null,null,null,null,null,null,"T-6",45200.973816642247,null,null,null,null,null,null,null,null,null,null,null,null,null,"T-6",45200.973816642247]
["Mass Flow",null,"g/s",null,null,null,{"$f":"SUM(Turbines!B2:B1048576)","v":69531.910467874113},null,null,null,null,null,null,null,"VLV-Dewar",464.5580341041059,null,null,null,null,null,null,null,null,null,null,null,null,null,"Expander gas losses",32799.961905253869]
["Mass Enthalpy",null,"kJ/kg",null,null,null,"Total UA in LNG",null,null,null,null,null,null,null,"VLV-HXVLP",869.94251833425369,null,null,null,null,null,null,null,null,null,null,null,null,null,"Expanders upstream valves",10246.836463335261]
["Mass Entropy",null,"kJ/kg-K",null,null,null,{"$f":"SUM(LNG!B2:B1048576)","v":558968.50897154154},null,null,null,null,null,null,null,"Mixer",1150.7107849803433,null,null,null,null,null,null,null,null,null,null,null,null,null,"JT valve",6477.2511054970091]
["Mass Heat capacity",null,"kJ/kg-K",null,null,null,null,null,null,null,null,null,null,null,"Piping",16101.523844996933,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mixer & Valves",467.60175816639094]
["Mass Density",null,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,"CC-100",32645.954450071946,null,null,null,null,null,null,null,null,null,null,null,null,null,"Subcooler",10129.9075178275]
["Molar Flow",null,"Nm3/h*",null,null,null,null,null,null,null,null,null,null,null,"CC-101",32765.954233335018,null,null,null,null,null,null,null,null,null,null,null,null,null,"LHe Dewar heat inleaks",6718.181818181818]
["Molar Enthalpy",null,"J/mol*",null,null,null,null,null,null,null,null,null,null,null,"CC-102",22878.555659351674,null,null,null,null,null,null,null,null,null,null,null,null,null,"2K Loop",574295.33905139146]
["Molar Entropy",null,"kJ/kgmole-C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RF Coupler",58517.646507180099]
["Molar Heat capacity",null,"kJ/kgmole-C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Thermal Shields",80300.599401837331]
["Molar Density",null,"kgmole/m3"]
["Volume Flow",null,"m3/h"]
["Dynamic Viscosity",null,"Pa-s"]
["Kinematic viscosity",null,"m²/s*"]
["Thermal conductivity",null,"W/m-K"]

{"sheet":"ExergyBalance","index":1,"n_rows":100,"n_cols":30,"rows_kept":100,"cut":false,"hidden":false,"merged":[[1,26,1,29],[1,4,1,6],[1,9,1,15],[1,16,1,19],[1,0,1,3],[1,7,1,8],[1,20,1,21],[1,22,1,23],[1,24,1,25]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turbine Bearing stream","Turbine Bearings","Turbine bearing +losses return stream","From Turbines 2"]
["Special Equipments",null,null,null,"Useful exergy destruction",null,null,"Heat Exchanger",null,"Compressors",null,null,null,null,null,null,"Turbines",null,null,null,"Valves",null,"Mixer",null,"Piping",null,"Additional circuits"]
["Name","ID","Type","Group","Name","ID","Group","Name","ID","Name","ID","Exergetic efficiency","Cooler","Electrical energy","In Coldbox","Group","Name","ID","Gas loss stream","Inlet valve","Name","ID","Name","ID","Name","ID","Name","ID IN","ID OUT","Production efficiency"]
["Adsobers","Ads80K",{"$f":"INDEX(_cT_Obj_Type,MATCH(B4,_cT_Obj,0))","v":"heaterop"},1,null,"2K Loops",null,null,"HX-01",null,"CC-100",null,null,"Q-CC100","YES",null,null,"T-1","T1_Loss","VLV-T1",null,"VLV-Dewar",null,"MIX-100",null,"PIPE-HP","Nitrogen",null,null,8]
[null,"ADS20K","heaterop",1,null,"TS",null,null,"HX-02",null,"CC-101",null,null,"Q-CC101","YES",null,null,"T-2","T2_Loss","VLV-T2",null,"VLV-HXVLP",null,"MIX-102",null,"PIPE-LP"]
["ORS","ORS","coolerop",null,null,"RF Coupler",null,null,"HX-03",null,"CC-102",null,null,"Q-CC102","YES",null,null,"T-3","T3_Loss","VLV-T3",null,null,null,"MIX-102-2",null,"PIPE-MP"]
["Dewar w Heat Loss","Subcooler","coolerop",2,null,null,null,null,"HX-04",null,"C-LP/MP",0.48,"MP Cooler",null,null,null,null,"T-4","T4_Loss","VLV-T4",null,null,null,"MIX-103-2-2",null,"PIPE-VLP"]
[null,"Dewar","tankop",2,null,null,null,null,"HX-05",null,"C-MP/HP",0.48,"HP Cooler",null,null,null,null,"T-5","T5_Loss","VLV-T5",null,null,null,"MIX-103-2-3"]
["WCS Bypass","VLV-LP/VLP","valveop",null,null,null,null,null,"HX-06",null,"C-VLP/LP",0.48,"E-104",null,null,null,null,"T-6","T6_Loss","VLV-T6",null,null,null,"MIX-103-8"]
[null,"VLV-HP/LP","valveop",null,null,null,null,null,"HX-07",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIX-103-8-2"]
["JT Valve","VLV-JT","valveop",null,null,null,null,null,"HX-08",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIX-105"]
[null,null,{"$error":"#N/A"},null,null,null,null,null,"HX-09",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIX-106"]
[null,null,{"$error":"#N/A"},null,null,null,null,null,"HX-10",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIX-107"]
[null,null,{"$error":"#N/A"},null,null,null,null,null,"HX-11",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIX-108"]
[null,null,{"$error":"#N/A"},null,null,null,null,null,"HX-12"]
[null,null,{"$error":"#N/A"},null,null,null,null,null,"HX-13"]
[null,null,{"$error":"#N/A"},null,null,null,null,null,"HX-VLP"]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$f":"INDEX(_cT_Obj_Type,MATCH(B36,_cT_Obj,0))","v":{"$error":"#N/A"}}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$f":"INDEX(_cT_Obj_Type,MATCH(B68,_cT_Obj,0))","v":{"$error":"#N/A"}}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$error":"#N/A"}]
[null,null,{"$f":"INDEX(_cT_Obj_Type,MATCH(B100,_cT_Obj,0))","v":{"$error":"#N/A"}}]

{"sheet":"TS Setup","index":3,"n_rows":53,"n_cols":111,"rows_kept":53,"cut":false,"hidden":false,"merged":[[35,34,49,34],[0,34,32,34]]}
["Trace isobars for",null,"Linewidth",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TURBINES","Linewidth",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linewidth",1,null,1,null,1,null,1,null,1,null,1.5,null,null,null,1054.7687862019407,null,533.39140793592901,null,374.72767113739394,null,266.66154838329493,null,123.8085799366345,null,63.647063161983347,null,37.91169591802452,null,26.384842000804408,null,20.827220083904226,null,17.844714652980791]
[19.5,null,"Linetype",null,null,null,null,null,null,null,null,null,null,null,null,"- . - . -",null,null,"--------",null,null,null,null,null,null,null,null,null,null,null,"- . . - . .",null,null,null,null,"Linetype","- . . - . .",null,null,null,"- . . - . .",null,null,null,"- . . - . .",null,null,null,"- . . - . .",null,null,null,"- . . - . .",null,null,null,"- . . - . .",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linetype","- - - - -",null,"- - - - -",null,"- - - - -",null,"- - - - -",null,"- - - - -",null,"- - - - -",null,null,null,199.99999999918285,19419.260163066952,99.999999999998437,15803.209839777599,69.999999990526987,13915.583411244015,49.999999998349153,12096.32474581992,24.999999999701629,8113.7997525704768,15.000000053486644,5047.1114440949796,10.000000997174652,2979.1677968531653,7.0000003772096875,1620.7157281548141,5.0000000296095095,693.21956212335942,3.5000342464003324,-2.6746973402306615]
[5,null,"Linecolor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linecolor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Linecolor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,200.15579781406379,19529.509995552769,100.13416620905963,15917.290180917127,70.108542783189733,14032.761264952189,50.076762568561605,12216.083959917298,25.030358162674986,8238.4786195658198,15.096948814351833,5179.0234533739658,10.212948398005608,3136.6548888959505,7.3398299032585328,1821.8301188979249,5.4912431452375472,957.03808462956658,4.1985925590362285,339.64802232428093]
[1.17,null,"Name","HP",null,null,"LP",null,null,"VLP",null,null,"MP",null,null,"Client",null,null,"Thermal Shields",null,null,"Last HX",null,null,"T1->T2",null,null,"T4->T5",null,null,"Cold Compressors",null,null,null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Name",{"$f":"OFFSET(INDIRECT(\"_Isobar_p\"),1,0) & \" barA\"","v":"19.5 barA"},null,{"$f":"OFFSET(INDIRECT(\"_Isobar_p\"),2,0) & \" barA\"","v":"5 barA"},null,{"$f":"OFFSET(INDIRECT(\"_Isobar_p\"),3,0) & \" barA\"","v":"1.17 barA"},null,{"$f":"OFFSET(INDIRECT(\"_Isobar_p\"),4,0) & \" barA\"","v":"0.027 barA"},null,{"$f":"OFFSET(INDIRECT(\"_Isobar_p\"),5,0) & \" barA\"","v":"0.49 barA"},null,"LV equilibrium",null,null,null,200.31167505498433,19645.516614358432,100.26849016468663,16037.123060435406,70.216946642959783,14155.337523360293,50.152427200355021,12341.203749605331,25.053573984184823,8368.5453828380068,15.181406572838171,5317.4177221079499,10.411784433626906,3297.4089354762687,7.6552218471665583,2019.6233553217855,5.9316403868229486,1204.3274265008222,4.7732452289087632,643.91328066575932]
[2.7E-2,null,"Streams","0HPa",{"$f":"INDEX(_TSData,MATCH(D5,_cT_Streams,0),1)","v":300},{"$f":"INDEX(_TSData,MATCH(D5,_cT_Streams,0),2)","v":23450.900749473647},"0LPa",{"$f":"INDEX(_TSData,MATCH(G5,_cT_Streams,0),1)","v":297.01679104003063},{"$f":"INDEX(_TSData,MATCH(G5,_cT_Streams,0),2)","v":29451.137342988823},"VLPa",{"$f":"INDEX(_TSData,MATCH(J5,_cT_Streams,0),1)","v":18.103381794872718},{"$f":"INDEX(_TSData,MATCH(J5,_cT_Streams,0),2)","v":16547.288860092744},"0MPc",{"$f":"INDEX(_TSData,MATCH(M5,_cT_Streams,0),1)","v":297.0167906089651},{"$f":"INDEX(_TSData,MATCH(M5,_cT_Streams,0),2)","v":26220.465179087536},"Supply 2K",{"$f":"INDEX(_TSData,MATCH(P5,_cT_Streams,0),1)","v":4.5},{"$f":"INDEX(_TSData,MATCH(P5,_cT_Streams,0),2)","v":1655.6308082427015},"To TS",{"$f":"INDEX(_TSData,MATCH(S5,_cT_Streams,0),1)","v":35.448082919989048},{"$f":"INDEX(_TSData,MATCH(S5,_cT_Streams,0),2)","v":12261.476194795749},"12MPb",{"$f":"INDEX(_TSData,MATCH(V5,_cT_Streams,0),1)","v":5.4348734949182358},{"$f":"INDEX(_TSData,MATCH(V5,_cT_Streams,0),2)","v":3107.4954305039482},"T1Lb",{"$f":"INDEX(_TSData,MATCH(Y5,_cT_Streams,0),1)","v":135.23484061663902},{"$f":"INDEX(_TSData,MATCH(Y5,_cT_Streams,0),2)","v":20345.521428864613},"T4Lb",{"$f":"INDEX(_TSData,MATCH(AB5,_cT_Streams,0),1)","v":14.475098012905278},{"$f":"INDEX(_TSData,MATCH(AB5,_cT_Streams,0),2)","v":10387.001255035748},"2K Return",{"$f":"INDEX(_TSData,MATCH(AE5,_cT_Streams,0),1)","v":3.8999999999999773},{"$f":"INDEX(_TSData,MATCH(AE5,_cT_Streams,0),2)","v":14573.435420728587},null,null,"ID","T-1",null,null,null,"T-2",null,null,null,"T-3",null,null,null,"T-4",null,null,null,"T-5",null,null,null,"T-6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300.00020368256702,23476.281291176314,300.00020062778378,26301.226324305775,300.00019175430805,29317.488202365475,300.00009362520842,37145.513552396755,300.00020427411351,31125.15391682414,3.5,886.9516100337861,null,null,200.46763108895485,19767.939439931906,100.40297849556407,16163.367197488562,70.325226170470614,14284.3180299039,50.227005568149309,12473.304551801839,25.069326162151498,8505.3692486465279,15.252294615758501,5458.5894977377247,10.59572944145873,3458.0893401629605,7.9480421010317741,2213.663024042547,6.3306828949018836,1435.8293384169208,5.2744024870094108,924.57904364590206]
[0.49,null,null,"1HPa",156.43316311985058,20074.432884357429,"1LPa",150.70739007286363,25877.327757395713,"0VLPA",290,31191.628839918041,"1MPa",150.70737349512612,22676.944555366044,"2K Return",3.8999999999999773,14573.435420728587,"From TS",50.551917080010952,14232.236775563182,"13MPa",4.4850000000000136,1640.1825448503516,"T2Ha",63.564068998623156,16411.936357367311,"T5Ha",12.150134108509008,9371.6217051300591,"CC1",6.9628598880015602,15303.280143511329,null,null,"Streams","1HPa",{"$f":"INDEX(_TSData,MATCH(AK6,_cT_Streams,0),1)","v":156.43316311985058},{"$f":"INDEX(_TSData,MATCH(AK6,_cT_Streams,0),2)","v":20074.432884357429},null,"T2Ha",{"$f":"INDEX(_TSData,MATCH(AO6,_cT_Streams,0),1)","v":63.564068998623156},{"$f":"INDEX(_TSData,MATCH(AO6,_cT_Streams,0),2)","v":16411.936357367311},null,"T3Hc",{"$f":"INDEX(_TSData,MATCH(AS6,_cT_Streams,0),1)","v":50.551917078098398},{"$f":"INDEX(_TSData,MATCH(AS6,_cT_Streams,0),2)","v":14232.079214296729},null,"8HPa",{"$f":"INDEX(_TSData,MATCH(AW6,_cT_Streams,0),1)","v":21.466215437194109},{"$f":"INDEX(_TSData,MATCH(AW6,_cT_Streams,0),2)","v":9410.6602541518969},null,"T5Ha",{"$f":"INDEX(_TSData,MATCH(BA6,_cT_Streams,0),1)","v":12.150134108509008},{"$f":"INDEX(_TSData,MATCH(BA6,_cT_Streams,0),2)","v":9371.6217051300591},null,"12HPa",{"$f":"INDEX(_TSData,MATCH(BE6,_cT_Streams,0),1)","v":6.9888849295174964},{"$f":"INDEX(_TSData,MATCH(BE6,_cT_Streams,0),2)","v":2453.4327316571848},null,null,{"$f":"INDEX(_TSData,MATCH(BI6,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(BI6,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,null,{"$f":"INDEX(_TSData,MATCH(BM6,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(BM6,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,null,{"$f":"INDEX(_TSData,MATCH(BQ6,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(BQ6,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,null,{"$f":"INDEX(_TSData,MATCH(BU6,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(BU6,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,null,237.17747256274967,22256.395227629619,231.30318061707629,24950.943481609142,224.78462103884488,27818.716042135267,237.27627522146415,35927.554487336689,220.80404430334724,29533.595728973502,3.6778947428653055,1055.3117170690764,null,null,200.62366526987506,19897.557700231104,100.53763804531667,16296.801232801454,70.433396865834254,14420.481488730011,50.300511861867591,12612.23585537874,25.077275895431939,8647.1762664375656,15.308415158623006,5604.0408754856899,10.76369984348662,3621.3977840354178,8.2193438218512824,2405.9088066392119,6.6946051923181926,1663.4433994556914,5.7207399895306708,1180.1193843240167]
[null,null,null,"2HPa",135.23484061663902,19319.416605308263,"2LPa",133.89598299229343,25255.017151312946,null,{"$error":"#N/A"},{"$error":"#N/A"},"2MPa",133.89597068421381,22054.416940167674,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},"CC2",12.436612471434785,16035.807624694762,null,null,null,"T1Ha",156.43316311985058,20074.432884357426,null,"T2Hb",63.569745412009922,16439.056120610563,null,"T3La",34.939378858739616,15001.747271684524,null,"8HPb",22.101261045659498,9584.2533041396873,null,"T5Hb",12.118419549907571,9433.2135426035638,null,"12HPb",7.0012139381660745,2468.6305301016509,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,187.52405357207002,21036.515201200073,178.34088299995204,23600.645183637556,168.4159651482893,26319.563973172306,187.66685191338016,34709.598833406497,162.51504762415223,27942.030099796233,3.855789485730611,1229.2957678160028,null,null,200.77977693840617,20035.301415563707,100.67247587884592,16438.354725275774,70.541475176009243,14564.757500350956,50.37296277284554,12759.255510412329,25.077067147801188,8797.1186761407862,15.348439630504174,5756.3349150855347,10.914261583313476,3787.3639630285388,8.4694583223011364,2597.0441440709842,7.0274396022307428,1880.0868887274062,6.1225707804709373,1427.685721476144]
["Tmin",null,null,"3HPa",63.564068998623156,15374.568089307071,"3LPa",60.544981859495863,21080.512023970448,null,{"$error":"#N/A"},{"$error":"#N/A"},"3MPa",60.544972850749275,17916.887615551674,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},"VLPA",18.103381794872718,16547.288860092744,null,null,null,"T1Hb",156.44236285742156,20090.652185366591,null,"T2La",50.046423415195676,16913.907628144876,null,"T3Lb",34.939378858739616,15001.747271684524,null,"T4Ha",22.100944510762588,9589.6267986062394,null,"T5La",7.8310111137867011,10164.334110009642,null,"12MPa",5.4348734949182358,3107.4954305039482,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,148.28876814581554,19816.653173661922,137.5133221807865,22250.351696514354,126.1892505513527,24820.581147320518,148.42963912998221,33491.639830940825,119.61291802425416,26350.3879116508,4.0336842285959165,1409.6375873311888,null,null,200.93596542184409,20182.29309929087,100.80749928887766,16589.149848987097,70.649478533976151,14718.268278584754,50.444377911518927,12915.486102166473,25.068328584370164,8956.2585877405309,15.370895658310076,5915.308962709375,11.045534306571483,3956.7369505603724,8.6980347315856079,2790.2925504635487,7.3316725567069625,2094.9232058302864,6.4862990096984277,1663.7600009306104]
[3.5,null,null,"4HPa",50.532970619770879,14160.82654479347,"4LPa",50.046423415195676,20079.436232545304,null,{"$error":"#N/A"},{"$error":"#N/A"},"4MPa",50.046559539717123,16913.921442215811,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"T1La",135.23484061663902,20345.521428864613,null,"T2Lb",50.046423415195676,16913.907628144876,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,"T4Hb",22.094840730879525,9606.2960215679341,null,"T5Lb",7.8310111137867011,10164.334110009642,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,117.29674339937716,18596.78516847625,106.04481987062638,20900.073783548371,94.553770207381547,23321.590304180387,117.39508143411979,32273.633365223985,88.044583273999876,24759.107116313866,4.211578971461222,1597.8668680058679,null,null,201.09223003399362,20339.904939011805,100.94271580273335,16750.55856058358,70.757425399335318,14882.385830583937,50.51477987975727,13082.299916989899,25.050676342841427,9124.8189901441547,15.374144469410851,6081.2554113003544,11.15518537095079,4130.6995543311778,8.9040063820451678,2981.1237275509843,7.6084657271243259,2307.457156973775,6.8158749506507661,1894.050412766089]
["Tmax",null,null,"5HPa",50.538570176605191,14173.350813791432,"5LPa",50.045996815185021,20079.391895290202,null,{"$error":"#N/A"},{"$error":"#N/A"},"5MPa",50.045991911919884,16905.804087972159,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,"T1Lb",135.23484061663902,20345.521428864613,null,"4MPb",50.046495225510796,16913.914718490156,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,"T4La",14.475098012905278,10387.001255035748,null,"11LPb",7.831011113783461,10164.322718217598,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,92.829607498695452,17376.856767082387,81.79500953012564,19549.766437770326,70.855493638891403,21822.616273239368,92.852405206212438,31055.790223904292,64.805477970589209,23167.393678878296,4.3894737143265843,1796.7055972111041,null,null,201.2485700750438,20509.838905841334,101.07813318933907,16924.282687279156,70.865335300494849,15058.812046942727,50.584194433595201,13261.399053458679,25.023718172803285,9305.1799213937193,15.356263005685889,6256.2776644709393,11.240267133386169,4310.2183115183852,9.0854640305029761,3175.7838071218971,7.8577797054497864,2519.6964170437936,7.113389438891943,2122.7445485146814]
[300,null,null,"6HPa",35.448082919989048,12261.476194795749,"6LPa",35.051685990578648,18186.079396171146,null,{"$error":"#N/A"},{"$error":"#N/A"},"6MPa",35.05168686782477,15026.775879666873,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,"T4Lb",14.475098012905278,10387.001255035748,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,73.532213543901378,16156.939385102383,63.116093242100447,18199.475476755724,53.104280526016197,20323.519749337825,73.439761369370444,29837.878477285976,47.705775707285767,21575.782935822583,4.5673684571918898,2010.9371326223688,null,null,201.40498483144461,20694.241793415651,101.21375946648607,17112.468937122703,70.973228878643624,15249.693699838559,50.652650645332386,13454.930421624935,24.987059051902236,9500.0185732455539,15.31521286853723,6442.5065909913037,11.297149673063529,4495.024604048017,9.2395660514048927,3374.0125746546387,8.0784143543834261,2733.8819650746855,7.3792511521430697,2346.1919906252774]
[null,null,null,"7HPa",35.296250494304672,12240.047692438528,"7LPc",{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},"7MPa",{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,58.332405969926441,14937.050178440973,48.737413930485957,16849.184458751639,39.814484775527148,18824.677614387201,58.085057523083691,28619.895781822888,35.124799911120249,19984.209755416479,4.7452632000571953,2249.6445297437608,null,null,201.56147357578433,20895.875227091754,101.34960290835915,17317.878898263127,71.081127933735161,15457.792434076098,50.720181065432769,13665.655713738553,24.94030777717677,9711.1752764223111,15.248497468715414,6642.5341375275539,11.321345130791258,4692.0910547514623,9.3622152385476056,3577.8566536601629,8.267688064697893,2948.4651672300502,7.6123324857317698,2571.7302817562768]
["Trace LV equilibrium",null,null,"8HPa",21.466215437194109,9410.6602541518969,"8LPa",19.413272047098701,15079.912171646312,null,{"$error":"#N/A"},{"$error":"#N/A"},"T3Lb",34.939378858739616,15001.747271684524,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,46.38192771675125,13717.161761159621,37.681860023336725,15499.102362525242,29.866809008650193,17325.733856299124,45.941296984342955,27401.960583124619,25.871042487143313,18392.709454580403,4.9231579429225008,2533.4231825556558,null,null,201.7180355666691,21118.375534903538,101.48567205334598,17544.14875807492,71.189055472735987,15686.744346035439,50.786821885138778,13897.210835934386,24.883084436569135,9942.5855175915985,15.153197374983563,6858.9259428522646,11.30745105589375,4900.4822761063033,9.4476956961234464,3789.3352294083243,8.4212722764291925,3167.9076166647114,7.8095819218331144,2801.7756856319088]
["YES",null,null,"9HPa",14.475098012905278,6927.0214767568941,"9LPa",14.335697125730405,13471.141184417247,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,37.009528984148403,12497.294809374604,29.191486803858226,14148.66034312752,22.426793814357268,15826.753433135043,36.336758183454862,26184.041014124719,19.066855223886307,16801.080567233435,5.1010526857878062,2930.6911236820624,null,null,201.87467004860207,21366.66727510692,101.62197571215131,17796.202955323755,71.297035760438348,15941.473693470805,50.852613101314091,14154.519530093166,24.815027669571208,10199.15624317189,15.025818239803641,7097.950583175817,11.248860340690442,5124.0129169840893,9.4881552689531645,4011.3592955486156,8.5324059918571038,3394.8457778372526,7.9655344566796771,3034.0361217320215]
[null,null,null,"10HPa",12.150134108509008,5730.8001623019654,"10LPa",10.556487412753938,11821.851968152125,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,29.681898865161912,11277.436854385021,22.690149841718949,12798.493336505062,16.86846408874095,14327.513093703563,28.740280234138766,24966.089847978976,14.068331143304647,15209.524515127883,5.190000057220459,3266.60040337092,null,null,202.03137625186591,21647.654306987872,101.75852297622188,18080.944961766476,71.405094373148415,16228.883357116945,50.917598685676637,14444.48336249559,24.7358006696563,10487.766568805489,14.862184553156339,7364.5965980570309,11.137447876670535,5367.977663970898,9.4729291827785573,4248.8694019686163,8.5909336580499485,3632.802952451797,8.071328013298853,3275.1489242624116]
["# of data points",null,null,"11HPa",7.9237944138031366,3047.6654919349044,"11LPa",7.8310111137867011,10164.334110009642,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,23.973750380333769,10057.600085141139,17.728817592924401,11448.062339846387,12.72650440056259,12828.777121494422,22.733078813775052,23748.320346259745,10.40115310175463,13618.013881834799,5.0121053143551535,5028.7046216603803,null,null,202.18815339240541,21971.447031582273,101.89532322651092,18408.484457892904,71.513258255627932,16559.081807938826,50.98182676138515,14777.20806990639,24.645094294528207,10818.488056658607,14.657407416942078,7667.2017276027727,10.962783927295447,5640.3363731186082,9.3875815980058519,4505.5848693464268,8.5818551601122408,3886.9300230736967,8.1129110931916557,3529.7450155531196]
[20,null,null,"12HPa",6.9888849295174964,2453.4327316571848,"12LPa",5.3348967307537123,7834.2394159391242,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,19.541863246480432,8837.5974379993731,13.967880885005286,10097.744143288506,9.6501553143139631,11329.847407477202,17.980633741354666,22530.168876443051,7.7178548580165511,12026.448228059951,4.834210571489848,5502.0837865444337,null,null,202.34500067171192,22353.718367014691,102.03238614258908,18794.492864138869,71.621555781672043,16947.737929243671,51.04534979075342,15168.356838623378,24.542625397927281,11206.925390683646,14.406006740849364,8025.3507992632149,10.710485158933693,5953.6000696251876,9.2127263364519081,4793.6596263179708,8.4828921766160761,4165.6975274288216,8.068134549288061,3807.3781964332816]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},"13LPd",4.3831043620451169,6275.8991253299582,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,16.104387844966539,7617.7066017732104,11.151519137961316,8747.4492391847434,7.3846745311516884,9830.8453545463981,14.222181514346801,21311.978046214652,5.7679245453501267,10434.843348218954,4.6563158286245425,5844.8002293510572,null,null,202.50191727670966,22820.721223805373,102.16972171212456,19265.220218648028,71.730016818770366,17421.096809168921,51.108224791913074,15644.70360200986,24.428128354989923,11679.201554234935,14.102247664161325,8459.7357483471733,10.35936607211795,6329.0155542730308,8.9207324280502576,5129.7649513678543,8.2613442394966796,4482.2690015431008,7.9019900143618429,4113.4480211724549]
["Reference stream",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,13.414905259129114,6397.8466096348047,9.0984157323792942,7397.2008714061176,5.7527924996554702,8331.6678257777112,11.251644999559574,20094.518050666829,4.3788230996599964,8843.2643935091837,4.478421085759237,6134.216013986329,null,null,202.65890237964308,23421.660061359038,102.30734024073445,19869.865275437445,71.838672806616245,18028.74016764294,51.170513520927102,16254.59082282011,24.30133803229262,12286.168841465302,13.740646685190768,9019.8055616389938,9.8784442456949364,6809.7056702873488,8.4657845819772319,5549.845423705252,7.8660904644222001,4866.5566221032059,7.5586601082537186,4480.4408466277418]
["0HPa",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,11.242121376534953,5178.0412980988867,7.6861986581658357,6046.8898926044048,4.6529582590595737,6832.880599044458,8.9015042978036263,18876.516010036637,3.534023921628318,7251.6994045079346,4.3005263428938747,6396.3027859649292,null,null,202.81595513766496,24266.954305732499,102.44525236236672,20718.845633023109,71.947556799169433,18880.452952772641,51.232282783148719,17108.822720578402,24.161962207759103,13135.896508981075,13.316324303597071,9817.3514983647001,9.2285307884175154,7495.3812599815046,7.7596123328524982,6130.9033818614262,7.1948454763582959,5386.1485080600323,6.9325986068511156,4963.9956188404385]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,9.3382212368863406,3958.0352501420653,6.7818199863723976,4696.6059837383018,4.3793428597504089,5333.9042602275249,7.0432802104252801,17658.454133966592,3.533101263235551,5660.1360060578463,4.1226316000285692,6643.8168936614029,null,null,202.97307469457749,25708.680327241625,102.58346905981551,22164.518629434868,72.056703588619087,20328.576781301508,51.293604690080059,18559.457981886557,24.009643969601598,14581.365204385509,12.824530057118011,11200.270648044409,8.3762238332463426,8726.4409896607885,6.6604682861265587,7180.7813624913915,6.0005291628951909,6301.1636273213489,5.7260362503994315,5791.2020365461358]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Show in textbox",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.4537438302157284,2738.1428555376765,6.1086711684970396,3346.0637598241519,4.3762267122681351,3834.9304712499029,5.5745602581633307,16440.441628785986,3.5348947124123242,4068.5726076221763,3.9447368571632637,6884.6220895215929,null,null,203.13026017536171,39086.921558354814,102.72200164101403,35546.508730250353,72.166149764943327,33713.237674473086,51.354557004044523,31946.623371977992,23.843913333654996,27962.675273133373,12.258537709861685,24507.676541075409,7.3032909650354441,21817.815283267839,5.0844671949438407,19935.526517636979,4.0152310683839119,18706.77305015994,3.441873681289735,17903.342122905691]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Name",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.4847846541672425,1518.2693858446464,5.0616744515771757,1995.9765822373372,4.3794196415647662,2335.9566823279297,4.4145901327808588,15222.566853225857,3.5356599833077098,2477.0092091792972,3.7668421142979582,7124.320786896561]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Power","X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.49996263449151,298.34010843276837,3.4999994291257508,645.68697558409087,3.4999799321997784,836.96429311789905,3.5000147821328937,14004.572756122763,3.4999891795268354,885.43527811221827,3.5889473714326527,7367.4757804497549]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"h is","X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X"]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"DHs","X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X"]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Mass flow","X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X",null,null,null,"X"]
["Trace Isenthalpes",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Molar flow"]
["YES",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Vol. flow"]
["# of data points",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"T IN"]
[20,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"T OUT"]
["Trace isobars between",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"p IN"]
[50,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"p OUT"]
[4.0000000000000001E-3,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"}]
["Start temperature",null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"}]
[200,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,"VALVES","Linewidth"]
[100,null,null,null,{"$f":"INDEX(_TSData,MATCH(D37,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(D37,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,{"$f":"INDEX(_TSData,MATCH(G37,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(G37,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,{"$f":"INDEX(_TSData,MATCH(J37,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(J37,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$f":"INDEX(_TSData,MATCH(P37,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(P37,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$f":"INDEX(_TSData,MATCH(AE37,_cT_Streams,0),1)","v":{"$error":"#N/A"}},{"$f":"INDEX(_TSData,MATCH(AE37,_cT_Streams,0),2)","v":{"$error":"#N/A"}},null,null,"Linetype","--------"]
[70,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Linecolor"]
[50,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"Name","JT Valve"]
[25,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,"ID","VLV-JT",{"$f":"MATCH(AK40,TSAuxData!$A$1:$A$100,0)","v":2},null,null,null,{"$f":"MATCH(AO40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(AS40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(AW40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(BA40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(BE40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(BI40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(BM40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(BQ40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}},null,null,null,{"$f":"MATCH(BU40,TSAuxData!$A$1:$A$100,0)","v":{"$error":"#N/A"}}]
[15,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AL$40-1,AK41)","v":4.4850060380985042},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AL$40-1,AK41+10)","v":1644.9860517648883},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AP$40-1,AO41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AP$40-1,AO41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AT$40-1,AS41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AT$40-1,AS41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AX$40-1,AW41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),AX$40-1,AW41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BB$40-1,BA41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BB$40-1,BA41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BF$40-1,BE41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BF$40-1,BE41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BJ$40-1,BI41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BJ$40-1,BI41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BN$40-1,BM41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BN$40-1,BM41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BR$40-1,BQ41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BR$40-1,BQ41+10)","v":{"$error":"#N/A"}},null,1,{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BV$40-1,BU41)","v":{"$error":"#N/A"}},{"$f":"OFFSET(INDIRECT(\"TSAUXDATA!A1\",TRUE),BV$40-1,BU41+10)","v":{"$error":"#N/A"}}]
[10,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,2,4.4961059633540685,1674.931688886958,null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"},null,2,{"$error":"#N/A"},{"$error":"#N/A"}]
[7,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,3,4.505455784393007,1711.944299532802,null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"},null,3,{"$error":"#N/A"},{"$error":"#N/A"}]
[5,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,4,4.5128903254884563,1744.0178928511179,null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"},null,4,{"$error":"#N/A"},{"$error":"#N/A"}]
[3.5,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,5,4.5182321292326151,1778.6940945671863,null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"},null,5,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,6,4.5212621810092628,1815.1441831339769,null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"},null,6,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,7,4.5217251519044908,1854.8834525899151,null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"},null,7,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,8,4.519299568386657,1888.8560249865129,null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"},null,8,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,9,4.5136015948709201,1925.1964732826946,null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"},null,9,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,null,null,10,4.3988305920880748,1964.5414125084471,null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"},null,10,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"}]
[null,null,null,null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"},null,{"$error":"#N/A"},{"$error":"#N/A"}]

{"sheet":"LNG","index":5,"n_rows":15,"n_cols":55,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Name","UA","LMTD","Cold Pinch Temperature","DT min","Duty","Heat Leak",null,"Stream Names","Duty","Pressure Drop","Mass flow","Composition","In Temperature","In Pressure","In liquid fraction","Out Temperature","Out Pressure","Out Liquid Fraction",null,"Stream Names","Duty","Pressure Drop","Mass flow","Composition","In Temperature","In Pressure","In liquid fraction","Out Temperature","Out Pressure","Out Liquid Fraction",null,"Stream Names","Duty","Pressure Drop","Mass flow","Composition","In Temperature","In Pressure","In liquid fraction","Out Temperature","Out Pressure","Out Liquid Fraction",null,"Stream Names","Duty","Pressure Drop","Mass flow","Composition","In Temperature","In Pressure","In liquid fraction","Out Temperature","Out Pressure","Out Liquid Fraction"]
["HX-01",139247.29694363067,4.1974235645526505,297.01679060896686,2.9832093910331423,584.47988549145566,139,"HOT","0HPa ~ 1HPa",584.47888549145557,50,783.9420391413571,"Helium:1",300,19.740000000000002,0,156.43316311985058,19.690000000000001,0,"COLD","1MPa ~ 0MPc",279.8482664833499,50,368.35255834067618,"Helium:1",150.70737349512612,5.12,0,297.0167906089651,5.07,0,"COLD","1LPa ~ 0LPa",304.77161900810586,26.541303012121972,401.16391648406335,"Helium:1",150.70739007286363,1.096541303012122,0,297.01679104003063,1.07,0]
["HX-02",22250.083130273695,3.0186403744503725,133.89597068421381,1.3388699324252116,67.164999271921303,22,"HOT","1HPb ~ 2HPa",67.164999271921431,20,609.30799242453509,"Helium:1",156.43316311985058,19.690000000000001,0,135.23484061663902,19.670000000000002,0,"COLD","2MPa ~ 1MPa",32.165256259143632,20,368.35255834067618,"Helium:1",133.89597068421381,5.14,0,150.70737349512612,5.12,0,"COLD","2LPa ~ 1LPa",35.021743012777506,4.2007817717027578,401.16391648406335,"Helium:1",133.89598299229343,1.100742084783825,0,150.70739007286363,1.096541303012122,0]
["HX-03",145275.85172851509,2.0185621183252236,133.89597068819975,1.3388699284392658,293.24833100661249,145,"HOT","T1Lb ~ T2Ha",65.121731253908337,20,174.33404671682214,"Helium:1",135.23484061663902,12,0,63.564068998623156,11.98,0,"HOT","2HPa ~ 3HPa",228.12608719985701,20,609.30799242453509,"Helium:1",135.23484061663902,19.670000000000002,0,63.564068998623156,19.650000000000002,0,"COLD","3MPa ~ 2MPa",140.5427166675675,20,368.35255834067618,"Helium:1",60.544972850749275,5.16,0,133.89597068421381,5.14,0,"COLD","3LPa ~ 2LPa",152.85112689189214,27.686970768040908,401.16391648406335,"Helium:1",60.544981859495863,1.1284290555518657,0,133.89598299229343,1.100742084783825,0]
["HX-04",30515.389416351507,1.3786075465759122,50.046495225510796,0.48647539426008279,42.068746136084911,31,"HOT","3HPa ~ 4HPa",42.068758091497131,20,609.30799242453509,"Helium:1",63.564068998623156,19.650000000000002,0,50.532970619770879,19.63,0,"COLD","4MPb ~ 3MPa",20.201312801964363,20,368.35255834067618,"Helium:1",50.046495225510796,5.18,0,60.544972850749275,5.16,0,"COLD","4LPb ~ 3LPa",21.898421378708335,5.9192834055811598,401.16391648406335,"Helium:1",50.046423415195676,1.1343483389574469,0,60.544981859495863,1.1284290555518657,0]
["HX-05","---",0.491804573278813,50.046559539721812,0.491804573278813,1.0000000000078561E-3,0,"HOT","4HPb ~ 5HPa",1.0000000000047748E-3,20,609.30799242453509,"Helium:1",50.538364113000625,19.54,0,50.538570176605191,19.52,0,"COLD","5MPa ~ 4MPa",1.0985409844721516E-4,20,194.31851162385408,"Helium:1",50.045991911919884,5.2,0,50.046559539717123,5.18,0,"COLD","5LPa ~ 4LPa",8.9014590156466511E-4,0,401.16391648406335,"Helium:1",50.045996815185021,1.1343483389574469,0,50.046423415195676,1.1343483389574469,0]
["HX-06",112454.4401810558,0.4135461920929776,38.341346550760903,0.38436662101389629,46.505105520823165,113,"HOT","5HPb ~ 6HPa",46.505105520823193,20,571.45322654407516,"Helium:1",50.538570176605191,19.52,0,35.448082919989048,19.5,0,"COLD","6MPa ~ 5MPa",15.303394580294857,20,194.31851162385408,"Helium:1",35.05168686782477,5.22,0,50.045991911919884,5.2,0,"COLD","6LPa ~ 5LPa",31.3147109405283,21.576742736473257,401.16391648406335,"Helium:1",35.051685990578648,1.1559250816939202,0,50.045996815185021,1.1343483389574469,0]
["HX-07",904.63507584032027,0.38173239266285236,34.939378858739616,0.35687163556505652,0.34532851198726633,5,"HOT","6HPb ~ 7HPa",0.34532955973504897,20,414.689480800681,"Helium:1",35.448082919989048,19.5,0,35.296250494304672,19.48,0,"COLD","T3Lb ~ 6MPa",0.11545039757960751,20,194.31851162385408,"Helium:1",34.939378858739616,5.24,0,35.05168686782477,5.22,0,"COLD","7LPa ~ 6LPa",0.23487706665987673,0.95472312993244501,401.16391648406335,"Helium:1",34.939378858739616,1.1568798048238527,0,35.051685990578648,1.1559250816939202,0]
["HX-08",36388.036682601254,0.894368669433942,34.939378858739616,0.35687163678434786,32.544319951131556,36,"HOT","7HPa ~ 8HPa",32.543818903383766,20,414.689480800681,"Helium:1",35.296250494304672,19.48,0,21.466215437194109,19.46,0,"COLD","8LPa ~ 7LPa",32.580820998879368,6.8740065355136046,401.16391648406335,"Helium:1",19.413272047098701,1.1637538113593662,0,34.939378858739616,1.1568798048238527,0]
["HX-09",13553.813035304502,0.79382114623443567,14.335697125730405,0.13940088717487242,10.759303399532655,14,"HOT","8HPd ~ 9HPa",10.759803399532661,20,225.06391648406338,"Helium:1",22.100944510762588,19.414999999999999,0,14.475098012905278,19.395,0,"COLD","9LPa ~ 8LPa",10.772803399532648,2.6732247638108459,401.16391648406335,"Helium:1",14.335697125730405,1.166427036123177,0,19.413272047098701,1.1637538113593662,0]
["HX-10",13631.901389157219,0.596356657369014,14.335697125730405,0.13940088717487242,8.129475146021818,14,"HOT","T4Lb ~ T5Ha",4.5502758328680599,20,335,"Helium:1",14.475098012905278,4.8239999999999998,0,12.150134108509008,4.8040000000000003,0,"HOT","9HPa ~ 10HPa",3.5791463218012307,20,225.06391648406338,"Helium:1",14.475098012905278,19.395,0,12.150134108509008,19.375,0,"COLD","10LPa ~ 9LPa",8.1435281373743464,2.6732247638108459,401.16391648406335,"Helium:1",10.556487412753938,1.1691002608869878,0,14.335697125730405,1.166427036123177,0]
["HX-11",9278.2289064799061,0.6512339854173711,7.831011113783461,9.2783300019675607E-2,6.0422979883815664,9,"HOT","10HPa ~ 11HPa",6.0423263515080636,20,225.06391648406338,"Helium:1",12.150134108509008,19.375,0,7.9237944138031366,19.355,0,"COLD","11LPb ~ 10LPa",6.0512696252550704,1.7185016338784012,401.16391648406335,"Helium:1",7.831011113783461,1.1708187625208664,0,10.556487412753938,1.1691002608869878,0]
["HX-12",1717.8852547690799,0.58076684093067532,7.8310111137867011,9.2783300016435533E-2,0.99769079249362691,5,"HOT","11HPa ~ 12HPa",0.99768179797184375,10,225.06391648406338,"Helium:1",7.9237944138031366,19.355,0,6.9888849295174964,19.344999999999999,0,"COLD","12LPa ~ 11LPa",1.00269978701541,0.95472312993244501,66.563916484063398,"Helium:1",5.3348967307537123,1.1717734856507986,0,7.8310111137867011,1.1708187625208664,0]
["HX-13",2249.4362439221968,0.21945120220932091,5.3348967307537123,9.9976764164523502E-2,0.49364148802194535,5,"HOT","12MPb ~ 13MPa",0.49364148802194546,10,66.563916484063398,"Helium:1",5.4348734949182358,3.0100000000000002,0,4.4850000000000136,3,1,"COLD","13LPd ~ 12LPa",0.49864148802194519,0.95472312993244501,66.563916484063398,"Helium:1",4.3831043620451169,1.1727282087807311,1.9330441195173353E-3,5.3348967307537123,1.1717734856507986,0]
["HX-VLP",31501.510983640172,6.6839231716181953,45.151180931184655,5.000440972761254,210.55367920453762,21,"HOT","HPa ~ HPb",210.5536784786355,100,145.67443568338243,"Helium:1",300,19.740000000000002,0,23.938158452081126,19.64,0,"COLD","VLPa ~ 0VLPa",210.57467993043977,50,149.1,"Helium:1",18.103381794872718,0.48599999999999993,0,290,0.43599999999999994,0]

{"sheet":"CoolerHeater","index":6,"n_rows":12,"n_cols":15,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Type","Name","Power","Mass Flow","Molar Flow","Feed Volume Flow","Molar composition","Pressure Drop","Delta T","Feed Temperature","Feed Pressure","Feed Liquid Fraction","Product Temperature","Product Pressure","Product Liquid Fraction"]
["Cooler","E-104",140093.26506792821,149.1,3005.4722874438639,1.3219914043502929,"Helium:1",50,-180.94960900980499,477.96640004983561,1.1200000000000001,0,297.01679104003063,1.07,0]
["Cooler","HP Cooler",1530698.5393477054,987.23347920076174,19900.086270789259,0.60698227313284037,"Helium:1",0,-298.69534296004338,598.69534296004338,20.309999999999999,0,300,20.309999999999999,0]
["Cooler","MP Cooler",1095352.1871059751,618.88092086008555,12475.046659106147,1.6491766495030511,"Helium:1",0,-340.87775770717303,640.87775770717303,5,0,300,5,0]
["Cooler","ORS",181.78096537531019,987.23347920076196,19900.086270789267,0.30569575589004661,"Helium:1",500,-4.3560303940921585E-3,300,20.309999999999999,0,299.99564396960591,19.809999999999999,0]
["Cooler","Subcooler",1158.5668487576668,157.69999999999999,3178.8261551300957,1.6655326738346024E-3,"Helium:1",10,-0.93487349491823579,5.4348734949182358,3.0100000000000002,0,4.5,3,1]
["Heater","2K Loops",3518.0612651021456,149.1,3005.4722874438639,1.1507943892017636E-3,"Helium:1",2973,-0.60000000000002274,4.5,3,1,3.8999999999999773,2.6999999999999996E-2,0]
["Heater","Ads20K",5,560.36391648406322,11295.494445850842,1.3664023549954536E-2,"Helium:1",45,-3.1653489691052528E-4,22.101261045659498,19.46,0,22.100944510762588,19.414999999999999,0]
["Heater","Ads80K",10,609.30799242453509,12282.08105801473,3.4152353163167157E-2,"Helium:1",90,5.3934932297465821E-3,50.532970619770879,19.63,0,50.538364113000625,19.54,0]
["Heater","E-106",2716.0229035054899,30.399999999999988,612.78576484435575,0.15098378816707725,"Helium:1",120.8187625208663,17.213690514212487,279.8043455840895,1.1708187625208664,0,297.01803609830199,1.05,0]
["Heater","RF Coupler",13429.786152430661,8.6,173.35386768623226,6.6377141161201643E-5,"Helium:1",1950,295.5,4.5,3,1,300,1.05,0]
["Heater","TS",12757.5,156.76374574339414,3159.953678790524,6.2356538311210755E-3,"Helium:1",500,15.103834160021904,35.448082919989048,19.5,0,50.551917080010952,19,0]

{"sheet":"Compressors","index":7,"n_rows":7,"n_cols":12,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Name","Power","Isentropic efficiency","Mass Flow","Molar Flow","Feed Volume Flow","Compression Ratio","Molar composition","Feed Temperature","Feed Pressure","Product Temperature","Product Pressure"]
["CC-100",2361.4692932041776,0.7,149.1,3005.4722874438639,0.44383258837526895,3,"Helium:1",3.8999999999999773,2.6999999999999996E-2,6.9628598880015602,8.1000000000000003E-2]
["CC-101",4224.9887737807958,0.7,149.1,3005.4722874438639,0.26458147301524604,3,"Helium:1",6.9628598880015602,8.1000000000000003E-2,12.436612471434785,0.24299999999999997]
["CC-102",4384.1641807032656,0.7,149.1,3005.4722874438639,0.15797483192386963,2,"Helium:1",12.436612471434785,0.24299999999999997,18.103381794872718,0.48599999999999993]
["C-LP/MP",1104953.942311977,0.75,618.88092086008555,12475.046659106147,3.6408421871145271,4.7619047619047619,"Helium:1",297.25782225699589,1.05,640.87775770717303,5]
["C-MP/HP",1541278.4019836013,0.75,987.23347920076151,19900.086270789256,1.2285584516587613,4.0620000000000003,"Helium:1",298.88854265452545,5,598.69534296004338,20.309999999999999]
["C-VLP/LP",145556.27619838368,0.75,149.1,3005.4722874438639,2.1592722966555828,2.692307692307693,"Helium:1",290.00124702634298,0.41599999999999993,477.96640004983561,1.1200000000000001]

{"sheet":"Turbines","index":8,"n_rows":7,"n_cols":14,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Name","Power","Isentropic efficiency","Mass Flow","Molar Flow","Feed Volume Flow","Molar composition","DHs","Feed Temperature","Feed Pressure","Product Temperature","Product Pressure","Product Liquid Fraction","Gas losses"]
["T-1",19667.183547771616,0.77,174.63404671682216,3520.1729567510806,2.9570702012917716E-2,"Helium:1",146.30893860271615,156.44236285742156,19.54,135.23484061663902,12,0,0.3]
["T-2",12541.15210211981,0.76,174.33404671682214,3514.1257288085376,1.9948190031716946E-2,"Helium:1",94.686914196797076,63.569745412009922,11.83,50.046423415195676,5.18,0,0.3]
["T-3",16306.787739519286,0.77,194.61851162385406,3923.0083387596578,1.1257508653905244E-2,"Helium:1",108.85336973676252,50.551917078098398,19,34.939378858739616,5.24,0,0.3]
["T-4",12565.901224019965,0.78,335.30000000000007,6758.7850971155449,8.2513870781387305E-3,"Helium:1",48.063325601431984,22.094840730879525,19.265000000000001,14.475098012905278,4.8239999999999998,0,0.3]
["T-5",6385.5430144237971,0.78,334.99999999999994,6752.7378691730009,1.6948405725235378E-2,"Helium:1",24.44594086263627,12.118419549907571,4.6539999999999999,7.8310111137867011,1.1708187625208664,0,0.4]
["T-6",2065.3428400196358,0.73,225.06391648406338,4536.7093487352968,1.5977880307919069E-3,"Helium:1",12.575108851721239,7.0012139381660745,19.195,5.4348734949182358,3.0100000000000002,0,{"$f":"NA()","v":{"$error":"#N/A"}}]

{"sheet":"ExergyData","index":9,"n_rows":122,"n_cols":32,"rows_kept":122,"cut":false,"hidden":true,"merged":[]}
["Object type","Name","Ex IN-OUT","Materialstreams",null,null,null,null,"Energystreams",null,"LNG",null,"Turbine",null,"Compressor",null,"Pipe",null,"Cooler",null,"Heater",null,"Valve",null,"Mixer",null,"Tank",null,"SystemInlet",null,"SystemOutlet"]
["compressor","CC-100",30284.48515686777,"0HPa",-4289043.132673027,0.78394203914135707,300,23450.900749473647,"Q-100",1530698.5393477054,"HX-01",27456.970239330083,"T-1",33019.837760486058,"CC-100",30284.48515686777,"PIPE-HP",2069.064766430296,"E-104",33837.986883528996,"2K Loops",574295.33905139146,"VLV-Dewar",464.5580341041059,"MIX-100",0,"Dewar",84377.237766431237,"From Buffer",0,"LHe",0]
["compressor","CC-101",28540.965459554223,"0HPb",-5086045.8532544756,0.92961647482473952,300,23450.900749473647,"Q-101",1541278.4019836013,"HX-02",5654.2239399459213,"T-2",37375.987571531907,"CC-101",28540.965459554223,"PIPE-LP",6472.7201787750237,"HP Cooler",468405.1196214417,"Ads20K",898.33372134552337,"VLV-HP/LP",54366.353699490137,"MIX-102",17.890382705256343,null,null,"LevelCompensation",0,"To Buffer",0]
["compressor","CC-102",18494.391478648409,"0HPc",-5083976.7884880453,0.92961647482473952,299.99564396960591,23443.481687159732,"Q-102",1095352.1871059751,"HX-03",32657.416357344016,"T-3",61244.283271490014,"CC-102",18494.391478648409,"PIPE-MP",3198.4741396289319,"MP Cooler",363622.20049866242,"Ads80K",1877.8562838314101,"VLV-HXVLP",869.94251833425369,"MIX-102-2",-1.3709927739109844]
["compressor","C-LP/MP",-966108.38180798246,"0HPd",-5399078.2532347189,0.98723347920076221,299.99564396960591,23443.481687159736,"Q-111",145556.27619838368,"HX-04",9419.2320972122252,"T-4",91097.04065854731,"C-LP/MP",-966108.38180798246,"PIPE-VLP",4361.2647601626813,"ORS",15474.288842745125,"E-106",2174.2552250974113,"VLV-JT",6477.2511054970091,"MIX-103-2-2",0]
["compressor","C-VLP/LP",-121513.7959050904,"0HPe",-5383603.9643919738,0.98723347920076199,300,23391.84747161514,"Q-112",140093.26506792821,"HX-05",880.02648664452136,"T-5",79863.16003873467,"C-MP/HP",-1334946.991871356,null,null,"Subcooler",-67529.148430421919,"RF Coupler",58517.646507180099,"VLV-LP/VLP",0,"MIX-103-2-3",-2.1774864289909601E-2]
["compressor","C-MP/HP",-1334946.991871356,"0HPf",-4915198.8447705321,0.98723347920076177,598.69534296004338,26978.616093583772,"Q-115",1104953.942311977,"HX-06",9520.5106717431918,"T-6",45200.973816642247,"C-VLP/LP",-121513.7959050904,null,null,null,null,"TS",79925.64318135893,"VLV-T1",849.73265104473103,"MIX-103-8",-9.199301749933511]
["coolerop","Subcooler",-67529.148430421919,"0LPa",-2925574.1804615306,0.40116391648406335,297.01679104003063,29451.137342988823,"Q-117",2716.0229035054899,"HX-07",1008.6062102401629,null,null,null,null,null,null,null,null,null,null,"VLV-T2",1418.3694216595031,"MIX-103-8-2",1145.6057808902115]
["coolerop","ORS",15474.288842745125,"0LPb",-4012918.0127030807,0.55026391648406336,297.0167910396774,29451.137342982653,"Q-2K",3518.0612651021456,"HX-08",19572.098373377696,null,null,null,null,null,null,null,null,null,null,"VLV-T3",668.73428895458346,"MIX-105",4.636581240221858]
["coolerop","E-104",33837.986883528996,"0LPd",-4019390.7328818557,0.55026391648406336,297.01803609830199,29490.347135380289,"Q-4.5K",-32767,"HX-09",13824.346452806611,null,null,null,null,null,null,null,null,null,null,"VLV-T4",1676.7571377169807,"MIX-106",-0.65152771910652518]
["coolerop","HP Cooler",468405.1196214417,"0LPe",-1053506.49688574,0.14909999999999998,477.96640004983561,31826.633200603399,"Q-CC100",2361.4692932041776,"HX-10",15662.969471445773,null,null,null,null,null,null,null,null,null,null,"VLV-T5",6189.9796660871943,"MIX-107",0]
["coolerop","MP Cooler",363622.20049866242,"0LPf",-1087344.483769269,0.14909999999999998,297.01679104003063,29451.151908754546,"Q-CC101",4224.9887737807958,"HX-11",18310.295193345053,null,null,null,null,null,null,null,null,null,null,"VLV-T6",1026.1428119540797,"MIX-108",-6.1783627481054282]
["expandop","T-6",45200.973816642247,"0LPg",-1087344.483769269,0.14909999999999998,297.01679104003063,29451.151908754546,"Q-CC102",4384.1641807032656,"HX-12",6402.9448964056792,null,null,null,null,null,null,null,null,null,null,null,null,"MIX-Turb",59532.71803855992]
["expandop","T-3",61244.283271490014,"0LPh",-4520609.5521179093,0.6188809208600855,297.25782225699589,29494.537355186469,"Q-DewarLoad",1258.5668487576668,"HX-13",1812.7421743749292]
["expandop","T-4",91097.04065854731,"0MPa",-3554501.1703099268,0.6188809208600855,640.87775770717303,30242.368673641264,"Q-HL_Ads20K",5,"HX-VLP",68596.128651737003]
["expandop","T-5",79863.16003873467,"0MPb",-3918123.3708085893,0.61888092086008528,300,26301.222851973369,"Q-HL_Ads80K",10]
["expandop","T-1",33019.837760486058,"0MPc",-2328806.1013109647,0.36835255834067621,297.0167906089651,26220.465179087536,"Q-HL_HP",0]
["expandop","T-2",37375.987571531907,"0MPd",-2332004.5754505936,0.36835255834067621,297.02114867064051,26249.409135696547,"Q-HL_LP",0]
["heaterop","2K Loops",574295.33905139146,"0MPe",-6250145.8366418881,0.98723347920076154,298.88854265452545,26281.950733736361,"Q-HL_MP",0]
["heaterop","TS",79925.64318135893,"0VLPa",-1170659.0280306677,0.14909999999999998,290,31191.628839918041,"Q-HL_VLP",0]
["heaterop","E-106",2174.2552250974113,"0VLPb",-1175020.2927908304,0.14909999999999998,290.00124702634298,31289.130846628588,"Q-HL-Dewar",100]
["heaterop","RF Coupler",58517.646507180099,"0VLPc",-1175020.2927908304,0.14909999999999998,290.00124702634298,31289.130846628588,"Q-ORS",181.78096537531019]
["heaterop","Ads80K",1877.8562838314101,"10HPa",-376966.2709822774,0.22506391648406338,12.150134108509008,5730.8001623019654,"Q-RFCoupler",13429.786152430661]
["heaterop","Ads20K",898.33372134552337,"10LPa",-1401494.7717064782,0.40116391648406335,10.556487412753938,11821.851968152125,"Q-Subcooler",1158.5668487576668]
["Inlet stream","From Buffer",0,"11HPa",-201845.55812368932,0.22506391648406338,7.9237944138031366,3047.6654919349044,"Q-T1",19667.183547771616]
["Inlet stream","LevelCompensation",0,"11LPa",-200450.59743843516,6.6563916484063457E-2,7.8310111137867011,10164.334110009642,"Q-T2",12541.15210211981]
["lngop","HX-13",1812.7421743749292,"11LPb",-1208063.7636545452,0.40116391648406335,7.831011113783461,10164.322718217598,"Q-T3",16306.787739519286]
["lngop","HX-12",6402.9448964056792,"12HPa",-162721.13422228943,0.22506391648406338,6.9888849295174964,2453.4327316571848,"Q-T4",12565.901224019965]
["lngop","HX-01",27456.970239330083,"12HPb",-163747.27703424351,0.22506391648406338,7.0012139381660745,2468.6305301016509,"Q-T5",6385.5430144237971]
["lngop","HX-06",9520.5106717431918,"12LPa",-154923.22864062965,6.6563916484063401E-2,5.3348967307537123,7834.2394159391242,"Q-T6",2065.3428400196358]
["lngop","HX-11",18310.295193345053,"12MPa",-208948.25085088576,0.22506391648406338,5.4348734949182358,3107.4954305039482,"Q-TS",12757.5]
["lngop","HX-05",880.02648664452136,"12MPb",-61797.617922970494,6.6563916484063401E-2,5.4348734949182358,3107.4954305039482]
["lngop","HX-02",5654.2239399459213,"13LPa",-39467.482803506478,6.6563916484063401E-2,4.3999999999999773,1964.545024686086]
["lngop","HX-04",9419.2320972122252,"13LPb",-123844.72056993771,6.6563916484063401E-2,4.4003144185588212,6252.9447632887895]
["lngop","HX-07",1008.6062102401629,"13LPc",-123838.5422071896,6.6563916484063401E-2,4.400314407842643,6252.6353682955032]
["lngop","HX-08",19572.098373377696,"13LPd",-124303.10024129371,6.6563916484063401E-2,4.3831043620451169,6275.8991253299582]
["lngop","HX-09",13824.346452806611,"13MPa",-32990.231698009469,6.6563916484063401E-2,4.4850000000000136,1640.1825448503516]
["lngop","HX-03",32657.416357344016,"1HPa",-4079435.4871821399,0.78394203914135696,156.43316311985058,20074.432884357429]
["lngop","HX-10",15662.969471445773,"1HPb",-3170684.2123721805,0.60930799242453504,156.43316311985058,20074.432884357426]
["lngop","HX-VLP",68596.128651737003,"1LPa",-2800240.7644321909,0.40116391648406335,150.70739007286363,25877.327757395713]
["mixerop","MIX-100",0,"1MPa",-2217074.9016100862,0.36835255834067621,150.70737349512612,22676.944555366044]
["mixerop","MIX-Turb",59532.71803855992,"2HPa",-3099837.9756735153,0.60930799242453504,135.23484061663902,19319.416605308263]
["mixerop","MIX-105",4.636581240221858,"2K Return",-648872.53856845142,0.14909999999999998,3.8999999999999773,14573.435420728587]
["mixerop","MIX-102-2",-1.3709927739109844,"2LPa",-2760367.9394432483,0.40116391648406335,133.89598299229343,25255.017151312946]
["mixerop","MIX-106",-0.65152771910652518,"2MPa",-2180447.2659604182,0.36835255834067621,133.89597068421381,22054.416940167674]
["mixerop","MIX-107",0,"3HPa",-2606875.7439622949,0.60930799242453504,63.564068998623156,15374.568089307071]
["mixerop","MIX-108",-6.1783627481054282,"3LPa",-2410820.8184548845,0.40116391648406335,60.544981859495863,21080.512023970448]
["mixerop","MIX-102",17.890382705256343,"3MPa",-1863769.1290484234,0.36835255834067621,60.544972850749275,17916.887615551674]
["mixerop","MIX-103-2-2",0,"4HPa",-2427081.7749108407,0.60930799242453504,50.532970619770879,14160.82654479347]
["mixerop","MIX-103-2-3",-2.1774864289909601E-2,"4HPb",-2428959.6311946721,0.60930799242453504,50.538364113000625,14171.15441568582]
["mixerop","MIX-103-8",-9.199301749933511,"4LPa",-2312240.5942779444,0.40116391648406335,50.046423415195676,20079.436232545304]
["mixerop","MIX-103-8-2",1145.6057808902115,"4LPb",-2312240.5942779444,0.40116391648406335,50.046423415195676,20079.436232545304]
["Outlet stream","LHe",0,"4MPa",-935389.99654294574,0.19431851162385408,50.046559539717123,16913.921442215811]
["Outlet stream","To Buffer",0,"4MPb",-1773136.1520766967,0.36835255834067621,50.046495225510796,16913.914718490156]
["pipeseg","PIPE-LP",6472.7201787750237,"5HPa",-2429362.1160707609,0.60930799242453504,50.538570176605191,14173.350813791432]
["pipeseg","PIPE-HP",2069.064766430296,"5HPb",-2278431.9866680889,0.57145322654407515,50.538570176605191,14173.350813791432]
["pipeseg","PIPE-VLP",4361.2647601626813,"5LPa",-2312236.148471775,0.40116391648406335,50.045996815185021,20079.391895290202]
["pipeseg","PIPE-MP",3198.4741396289319,"5MPa",-934916.9007385592,0.19431851162385408,50.045991911919884,16905.804087972159]
["tankop","Dewar",84377.237766431237,"6HPa",-1997173.0162570698,0.57145322654407515,35.448082919989048,12261.476194795749]
["valveop","VLV-JT",6477.2511054970091,"6HPb",-1449299.0899525462,0.41468948080068102,35.448082919989048,12261.476194795749]
["valveop","VLV-Dewar",464.5580341041059,"6LPa",-2115692.2622298542,0.40116391648406335,35.051685990578648,18186.079396171146]
["valveop","VLV-T6",1026.1428119540797,"6MPa",-840681.30589771795,0.19431851162385408,35.05168686782477,15026.775879666873]
["valveop","VLV-LP/VLP",0,"7HPa",-1446978.5671572257,0.41468948080068102,35.296250494304672,12240.047692438528]
["valveop","VLV-HP/LP",54366.353699490137,"7LPa",-2113706.7393820584,0.40116391648406335,34.939378858739616,18167.629748174251]
["valveop","VLV-T3",668.73428895458346,"8HPa",-1127527.2237304938,0.41468948080068102,21.466215437194109,9410.6602541518969]
["valveop","VLV-T4",1676.7571377169807,"8HPb",-1550674.9738957579,0.56036391648406325,22.101261045659498,9584.2533041396873]
["valveop","VLV-T5",6189.9796660871943,"8HPc",-1551573.3076171034,0.56036391648406336,22.100944510762588,9589.6267986062412]
["valveop","VLV-T1",849.73265104473103,"8HPd",-623172.11200084281,0.22506391648406338,22.100944510762588,9589.6267986062394]
["valveop","VLV-T2",1418.3694216595031,"8LPa",-1774683.297581949,0.40116391648406335,19.413272047098701,15079.912171646312]
["valveop","VLV-HXVLP",869.94251833425369,"9HPa",-454155.00086435833,0.22506391648406338,14.475098012905278,6927.0214767568941]
[null,null,null,"9LPa",-1591841.8399926582,0.40116391648406335,14.335697125730405,13471.141184417247]
[null,null,null,"CC1",-679157.02372531919,0.14909999999999998,6.9628598880015602,15303.280143511329]
[null,null,null,"CC2",-707697.98918487341,0.14909999999999998,12.436612471434785,16035.807624694762]
[null,null,null,"From Buffer",0,0,300,29542.232614293389]
[null,null,null,"From Subcooler",-78878.768369150581,0.15769999999999998,4.5,1655.6308082427015]
[null,null,null,"From TS",-627799.56948588253,0.15676374574339413,50.551917080010952,14232.236775563182]
[null,null,null,"From Turbines",-219882.01077391292,3.039999999999999E-2,279.8043455840895,28954.146840982408]
[null,null,null,"From Turbines 2",-222056.26599901033,3.039999999999999E-2,297.01803609830199,29490.361548066059]
[null,null,null,"GHe Return",-62819.215359270747,8.5999999999999983E-3,300,29542.232614293389]
[null,null,null,"HPa",-797002.7205814484,0.14567443568338242,300,23450.900749473647]
[null,null,null,"HPb",-421132.20186603966,0.14567443568338242,23.938158452081126,10032.298406446811]
[null,null,null,"HPc",-422002.14438437391,0.14567443568338242,23.93215201849344,10052.204496220518]
[null,null,null,"HP-LPa",-161972.34759704149,2.9617004376022858E-2,299.99564396960591,23443.481687159732]
[null,null,null,"HP-LPb",-216338.70129653162,2.9617004376022858E-2,301.16275679975115,29562.303722551413]
[null,null,null,"LevelCompensation",0,0,4.4003144185588212,6252.9447632887895]
[null,null,null,"LHe",0,0,4.4003144185588212,1809.3262361102941]
[null,null,null,"LP-VLPa",0,0,297.01679104003063,29451.151908754546]
[null,null,null,"LP-VLPb",0,0,297.05750396914084,31413.959248640916]
[null,null,null,"Supply 2K",-74577.19951705994,0.14909999999999998,4.5,1655.6308082427015]
[null,null,null,"Supply LHe",-4301.5688520906469,8.6E-3,4.5,1655.6308082427015]
[null,null,null,"T1_Loss",-1619.307683025861,2.9999999999999997E-4,135.23484061663902,20345.521428864613]
[null,null,null,"T1Ha",-908751.27480996004,0.17463404671682212,156.43316311985058,20074.432884357426]
[null,null,null,"T1Hb",-909601.00746100477,0.17463404671682214,156.44236285742156,20090.652185366591]
[null,null,null,"T1La",-942620.84522149083,0.17463404671682214,135.23484061663902,20345.521428864613]
[null,null,null,"T1Lb",-941001.537538465,0.17433404671682215,135.23484061663902,20345.521428864613]
[null,null,null,"T2_Loss",-1444.1073912481261,2.9999999999999997E-4,50.046423415195676,16913.907628144876]
[null,null,null,"T2Ha",-800395.92770667188,0.17433404671682215,63.564068998623156,16411.936357367311]
[null,null,null,"T2Hb",-801814.29712833138,0.17433404671682215,63.569745412009922,16439.056120610563]
[null,null,null,"T2La",-839190.28469986329,0.17433404671682215,50.046423415195676,16913.907628144876]
[null,null,null,"T2Lb",-837746.17730861518,0.17403404671682215,50.046423415195676,16913.907628144876]
[null,null,null,"T3_Loss",-1295.8174072957211,2.9999999999999997E-4,34.939378858739616,15001.747271684524]
[null,null,null,"T3Ha",-150930.129402672,3.7854765880459926E-2,50.538570176605191,14173.350813791432]
[null,null,null,"T3Hb",-151598.86369162658,3.7854765880459926E-2,50.551917080010952,14232.236775563182]
[null,null,null,"T3Hc",-779389.23387575918,0.19461851162385407,50.551917078098398,14232.079214296729]
[null,null,null,"T3La",-840633.51714724919,0.19461851162385407,34.939378858739616,15001.747271684524]
[null,null,null,"T3Lb",-839337.6997399535,0.19431851162385408,34.939378858739616,15001.747271684524]
[null,null,null,"T4_Loss",-913.66685959963411,2.9999999999999997E-4,14.475098012905278,10387.001255035748]
[null,null,null,"T4Ha",-928401.19561626029,0.33529999999999999,22.100944510762588,9589.6267986062394]
[null,null,null,"T4Hb",-930077.95275397727,0.33530000000000004,22.094840730879525,9606.2960215679341]
[null,null,null,"T4La",-1021174.9934125246,0.33530000000000004,14.475098012905278,10387.001255035748]
[null,null,null,"T4Lb",-1020261.3265529249,0.33500000000000002,14.475098012905278,10387.001255035748]
[null,null,null,"T5_Loss",-1204.5601162090663,4.0000000000000002E-4,7.8310111137867011,10164.334110009642]
[null,null,null,"T5Ha",-922765.95762027113,0.33499999999999996,12.150134108509008,9371.6217051300591]
[null,null,null,"T5Hb",-928955.93728635833,0.33499999999999996,12.118419549907571,9433.2135426035638]
[null,null,null,"T5La",-1008819.097325093,0.33499999999999996,7.8310111137867011,10164.334110009642]
[null,null,null,"T5Lb",-1007614.5372088839,0.33459999999999995,7.8310111137867011,10164.334110009642]
[null,null,null,"T6_Loss",-742.71612834279017,8.0000000000000004E-4,5.4348734949182358,3107.4954305039482]
[null,null,null,"To Buffer",0,0,299.99564396960591,23443.481687159732]
[null,null,null,"To Subcooler",-146407.9167995725,0.15769999999999998,5.4348734949182358,3107.4954305039482]
[null,null,null,"To TS",-547873.9263045236,0.15676374574339413,35.448082919989048,12261.476194795749]
[null,null,null,"Turbine Bearings",-153129.11714963178,2.8000000000000001E-2,299.99564396960591,23443.481687159732]
[null,null,null,"VLPa",-726192.38066352182,0.14909999999999998,18.103381794872718,16547.288860092744]

{"sheet":"TSAuxData","index":10,"n_rows":12,"n_cols":63,"rows_kept":12,"cut":false,"hidden":true,"merged":[]}
["Valve","T1","T2","T3","T4","T5","T6","T7","T8","T9","T10","S1","S2","S3","S4","S5","S6","S7","S8","S9","S10",null,"Turbine","Up 1","Up 2","Up 3","Up 4","Up 5","Up 6","Down 1","Down 2","Down 3","Down 4","Down 5","Down 6"]
["VLV-JT",4.4850060380985042,4.4961059633540685,4.505455784393007,4.5128903254884563,4.5182321292326151,4.5212621810092628,4.5217251519044908,4.519299568386657,4.5136015948709201,4.3988305920880748,1644.9860517648883,1674.931688886958,1711.944299532802,1744.0178928511179,1778.6940945671863,1815.1441831339769,1854.8834525899151,1888.8560249865129,1925.1964732826946,1964.5414125084471,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,573.15955021783759,27247.432711396094]
["VLV-Dewar",4.400314407842643,4.3979881741438476,4.3993497813829663,4.3970321127995362,4.3947134068532137,4.3923936648471908,4.3900728880771567,4.3877510778326041,4.3854282353965459,4.3831043620447758,4.3807899759265183,4.3784729532674191,4.3761548724779686,4.3738357346722978,6263.09236050863,6265.6412788697944,6268.1963883165035,6270.7577149885046,6273.3252851778279,6275.89912532996,6278.479301543467,6281.0657970375096,6283.6586444491249,6286.2578708137344]
["VLV-T6",6.9888849295174964,6.9902636289805855,6.9916401323129094,6.9930144368228753,6.9943865398234379,6.995756438628348,6.9971241305516969,6.9984896129074627,6.9998528830084865,7.0012139381660745,2453.4327316571821,2455.1205440958238,2456.8085992461547,2458.4968339828683,2460.185270976624,2461.8739113787997,2463.5627563408325,2465.251807014231,2466.9410645505955,2468.6305301016491,null,"T-6","12HPb","12HPa",null,null,null,null,"12MPa","To Subcooler","From Subcooler","Supply 2K","2K Return","CC1"]
["VLV-LP/VLP",297.01679103872715,297.02131474730322,297.02583844364773,297.03036212886008,297.03488580058496,297.03940945998676,297.04393310002132,297.04845673547521,297.05298035852445,297.05750396914078,29451.137342966038,29597.282990327749,29754.484461947246,29924.565924139129,30109.798236000293,30313.167403437557,30538.537693339418,30791.46171360751,31079.488174176589,31413.959248640916,null,"T-3","T3Hc",null,null,null,null,null,"T3La","T3Lb"]
["VLV-HP/LP",299.99564396960591,300.12535405821762,300.25505790953707,300.38475489473961,300.5144443802364,300.64412572765968,300.77379829384711,300.90346143082706,301.0331144858045,301.16275679975121,23443.481687159732,23676.384721077513,23938.209501659381,24237.252753483561,24585.988563527055,25004.449569994238,25527.919198390828,26227.870014202068,27288.779121120046,29562.303722551405,null,"T-4","T4Hb","T4Ha","8HPc","8HPb",null,null,"T4La","T4Lb"]
["VLV-T3",50.538570176605191,50.540054923703877,50.541539229927338,50.543023095858388,50.544506522081178,50.545989509180913,50.54747205774413,50.548954168358648,50.550435841613307,50.551917078098398,14173.35081379143,14179.802028994152,14186.271526759007,14192.759416212517,14199.265807459969,14205.790811597104,14212.334540722082,14218.897107947534,14225.478627412873,14232.079214296729,null,"T-5","T5Hb","T5Ha",null,null,null,null,"T5La","T5Lb","11LPb"]
["VLV-T4",22.100944510762588,22.100269049636296,22.099592904807565,22.098916076083071,22.098238563269518,22.097560366173667,22.09688148460242,22.096201918362681,22.095521667261494,22.094840731105961,9589.6267986062376,9591.4702063759341,9593.3151003467592,9595.1614831403949,9597.0093573853082,9598.8587257167692,9600.7095907768489,9602.5619552144854,9604.4158216854739,9606.2711928525077,null,"T-1","T1Hb","T1Ha","1HPa",null,null,null,"T1La","T1Lb"]
["VLV-T5",12.150134108509008,12.146625632318887,12.143113319681618,12.139597168688113,12.136077177425989,12.132553343979339,12.129025666428959,12.125494142851835,12.121958771321488,12.118419549907571,9371.6217051300609,9378.3655416338279,9385.1338875484489,9391.9269182674161,9398.7448110394398,9405.5877449946238,9412.4559011711353,9419.3494625422863,9426.2686140441292,9433.2135426035657,null,"T-2","T2Hb","T2Ha",null,null,null,null,"T2La","T2Lb","4MPb"]
["VLV-T1",156.4331631198506,156.43418528686229,156.43520746033536,156.43622964027,156.43725182666643,156.43827401952478,156.43929621884536,156.44031842462823,156.44134063687375,156.44236285558199,20074.432884357426,20076.224106012105,20078.016818206881,20079.811023470691,20081.60672433893,20083.403923353442,20085.20262306256,20087.00282602114,20088.804534790532,20090.607751938674]
["VLV-T2",63.564068998623128,63.564699709371922,63.565330420395014,63.565961131704569,63.566591843312807,63.567222555231893,63.567853267474021,63.568483980051411,63.569114692976257,63.569745406260779,16411.936357367311,16414.901156419328,16417.869984722685,16420.84285352716,16423.819774129672,16426.8007578746,16429.785816153973,16432.774960407824,16435.768202124364,16438.76555284033]
["VLV-HXVLP",23.938158452081126,23.937494242057255,23.936829239642123,23.936163444629727,23.935496856814183,23.934829475989801,23.934161301950923,23.933492334492115,23.932822573408032,23.93215201849344,10032.298406446807,10034.501715377597,10036.707133727994,10038.914665885963,10041.124316252926,10043.336089243805,10045.549989287072,10047.766020824823,10049.984188312812,10052.204496220516]

{"sheet":"DS_HX_Template","index":11,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":true,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : "]
["OPERATING CONDITIONS"]
["Fluid",null,"Units"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[]
[]
[]
[]
["Liquid","inlet","%"]
["fraction","outlet","%"]
["Flowrate",null,"g/s"]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs"]
["pressure","outlet","bar abs"]
["Operating","inlet","K"]
["temperat.","outlet","K"]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",null,null,null,"","",""]
[null,null,null,null,null,null,"Heat leak",null,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"Streams Summary","index":12,"n_rows":122,"n_cols":26,"rows_kept":122,"cut":false,"hidden":false,"merged":[]}
["Name","Fluid Package","Property Package","Temperature","Pressure","Vapour fraction","Molecular weight","Mass","Flow","Composition","Enthalpy","Entropy","Heat capacity cp","Density","Molar","Flow","Composition","Enthalpy","Entropy","Heat capacity cp","Density","Volume Flow","Compressibility","Dynamic Viscosity","Kinematic viscosity","Thermal conductivity"]
["0HPa","Basis-He","MBWR",300,19.740000000000002,1,4.0029802322387695,null,783.9420391413571,"Helium:1",1564.1474650896414,23.450900749473647,5.1911378242510127,3.1396417935258278,null,15802.254014765806,"Helium:1",6261.2513830602156,93.873492128336352,20.780022093303778,0.78432607991419001,898.88959521702475,1.0090263366812275,8.5058331997752245E-5,2.7091731347553332E-3,0]
["0HPb","Basis-He","MBWR",300,19.740000000000002,1,4.0029802322387695,null,929.6164748247395,"Helium:1",1564.1474650896412,23.450900749473647,5.1911378242510127,3.1396417935258278,null,18738.675741361578,"Helium:1",6261.2513830602147,93.873492128336352,20.780022093303778,0.78432607991419001,1065.9239268218548,1.0090263366812275,8.5058331997752245E-5,2.7091731347553332E-3,0]
["0HPc","Basis-He","MBWR",299.99564396960591,19.809999999999999,1,4.0029802322387695,null,929.6164748247395,"Helium:1",1564.1474650896412,23.443481687159732,5.1911329756221605,3.1507205335984461,null,18738.675741361578,"Helium:1",6261.2513830602147,93.843793768552004,20.780002684338331,0.78709370289253833,1062.1758653874895,1.009058519407718,8.5053747578708384E-5,2.6995014845562419E-3,0]
["0HPd","Basis-He","MBWR",299.99564396960591,19.809999999999999,1,4.0029802322387686,null,987.23347920076219,"Helium:1",1564.1474650896412,23.443481687159736,5.1911329756221614,3.1507205335984456,null,19900.08627078927,"Helium:1",6261.2513830602138,93.843793768552004,20.780002684338331,0.78709370289253833,1128.0088117062119,1.009058519407718,8.5053747578708384E-5,2.6995014845562419E-3,0]
["0HPe","Basis-He","MBWR",300,20.309999999999999,1,4.0029802322387686,null,987.23347920076196,"Helium:1",1564.3315967760209,23.39184747161514,5.1910981018291853,3.2294641328152838,null,19900.086270789267,"Helium:1",6261.9884585609207,93.637103024419844,20.779863085234425,0.80676494647817021,1100.5047212041677,1.0092875430139239,8.505898836036245E-5,2.6338421751169075E-3,0]
["0HPf","Basis-He","MBWR",598.69534296004338,20.309999999999999,1,4.0029802322387686,null,987.23347920076174,"Helium:1",3114.8245364876266,26.978616093583774,5.1910616067959703,1.6264617978138254,null,19900.086270789259,"Helium:1",12468.581046452256,107.99486691577457,20.779716996337893,0.4063127228845157,2185.1361832782254,1.0041922985445795,9.9368386589629258E-4,6.1094817427125067E-2,0]
["0LPa","Basis-He","MBWR",297.01679104003063,1.07,1,4.0029802322387695,null,401.16391648406335,"Helium:1",1542.6260302503747,29.451137342988822,5.1925008744061811,0.17335956644823858,null,8086.4321510080299,"Helium:1",6175.1015048292156,117.89232060093329,20.785478356130469,4.3307624917069049E-2,8330.6051631931841,1.0004875155753372,8.1887384312168335E-5,4.7235572855806686E-2,0]
["0LPb","Basis-He","MBWR",297.0167910396774,1.07,1,4.0029802322387695,null,550.26391648406332,"Helium:1",1542.6260302485407,29.451137342982651,5.192500874406182,0.17335956644844458,null,11091.904438451893,"Helium:1",6175.1015048218742,117.89232060090859,20.785478356130472,4.3307624917120507E-2,11426.828873223694,1.0004875155753383,8.1887384312265724E-5,4.7235572855806734E-2,0]
["0LPd","Basis-He","MBWR",297.01803609830199,1.05,1,4.0029802322387695,null,550.26391648406332,"Helium:1",1542.6260302485407,29.49034713538029,5.1925023721246637,0.17012005391188251,null,11091.904438451893,"Helium:1",6175.1015048218742,118.04927662478653,20.785484351467947,4.2498349739973233E-2,11644.424356746946,1.0004783040142913,8.188863554214567E-5,4.8135792141567109E-2,0]
["0LPe","Basis-He","MBWR",477.96640004983561,1.1200000000000001,1,4.0029802322387695,null,149.1,"Helium:1",2482.2186866348088,31.8266332006034,5.1924853245180076,0.11278439444413545,null,3005.4722874438639,"Helium:1",9936.2723346928196,127.40138356072953,20.785416110235495,2.8175106520837819E-2,4759.1690556610547,1.000295586726393,4.6690993245267199E-4,0.41398451865070979,0]
["0LPf","Basis-He","MBWR",297.01679104003063,1.07,1,4.0029802322387695,null,149.1,"Helium:1",1542.6260302436067,29.451151908754547,5.1925008740433043,0.17335908042110304,null,3005.4722874438639,"Helium:1",6175.1015048021236,117.89237890740556,20.785478354677881,4.3307503500747371E-2,3096.2323905743333,1.000490320528387,8.188738430893805E-5,4.723570528294628E-2,0]
["0LPg","Basis-He","MBWR",297.01679104003063,1.07,1,4.0029802322387695,null,149.1,"Helium:1",1542.6260302436067,29.451151908754547,5.1925008740433043,0.17335908042110304,null,3005.4722874438639,"Helium:1",6175.1015048021236,117.89237890740556,20.785478354677881,4.3307503500747371E-2,3096.2323905743333,1.000490320528387,8.188738430893805E-5,4.723570528294628E-2,0]
["0LPh","Basis-He","MBWR",297.25782225699589,1.05,1,4.0029802322387686,null,618.88092086008555,"Helium:1",1543.8711184862952,29.49453735518647,5.1925022699126284,0.16998290204678346,null,12475.046659106147,"Helium:1",6180.0855684249973,118.06604999183938,20.785483942315185,4.2464087301204628E-2,13107.031873612297,1.0004778492139221,8.2138667123528286E-5,4.8321723028897173E-2,0]
["0MPa","Basis-He","MBWR",640.87775770717303,5,1,4.0029802322387686,null,618.88092086008555,"Helium:1",3329.2774948476394,30.242368673641263,5.1922248246156935,0.37526660412429064,null,12475.046659106147,"Helium:1",13327.03199951251,121.05960397666297,20.78437333427603,9.3746804219018889E-2,5937.0359382109837,1.0009481881978395,1.237222166072106E-3,0.32969151863626278,0]
["0MPb","Basis-He","MBWR",300,5,1,4.0029802322387686,null,618.88092086008533,"Helium:1",1559.3858239528295,26.301222851973368,5.1922031798303605,0.80060120462284023,null,12475.046659106147,"Helium:1",6242.1906277165408,105.28327516015597,20.78428669062821,0.20000128858370195,2782.8727988810551,1.0022803599923598,8.5042409707064353E-5,1.0622318479663976E-2,0]
["0MPc","Basis-He","MBWR",297.0167906089651,5.07,1,4.0029802322387695,null,368.35255834067618,"Helium:1",1543.9190381376752,26.220465179087537,5.1922040065150963,0.81991558869210457,null,7425.0396116831089,"Helium:1",6180.2773898422092,104.96000379199239,20.784289999830868,0.20482628969505196,1617.3240615436098,1.002338760010699,8.1891491112067022E-5,9.9877953586291653E-3,0]
["0MPd","Basis-He","MBWR",297.02114867064051,5,1,4.0029802322387695,null,368.35255834067618,"Helium:1",1543.9190381376752,26.249409135696549,5.192209145039782,0.80860952707105649,null,7425.0396116831089,"Helium:1",6180.2773898422092,105.07586587814104,20.784310569243608,0.20200187864001037,1639.9376530100001,1.0023063621213355,8.1895954873567885E-5,1.0127997770470404E-2,0]
["0MPe","Basis-He","MBWR",298.88854265452545,5,1,4.0029802322387686,null,987.23347920076151,"Helium:1",1553.614919456224,26.281950733736362,5.1922053618382478,0.80357062203090934,null,19900.086270789256,"Helium:1",6219.0898110944918,105.20612925181987,20.78429542516265,0.20074309025040873,4422.810425971541,1.002289996651244,8.3858062537223049E-5,1.0435680478871147E-2,0]
["0VLPa","Basis-He","MBWR",290,0.43599999999999994,1,4.0029802322387695,null,149.1,"Helium:1",1505.9861165584591,31.191628839918042,5.1925497747427425,7.2369745867047225E-2,null,3005.4722874438639,"Helium:1",6028.4326546095435,124.85947365752062,20.785674103211075,1.8078966586995256E-2,7416.9114948406595,1.0002030020422894,7.4820301889031506E-5,0.10338616087789818,0]
["0VLPb","Basis-He","MBWR",290.00124702634298,0.41599999999999993,1,4.0029802322387695,null,149.1,"Helium:1",1505.9861165584591,31.289130846628588,5.1925512161922347,6.9051041052550652E-2,null,3005.4722874438639,"Helium:1",6028.4326546095435,125.24977226298655,20.785679873304897,1.7249908080093638E-2,7773.3802679600985,1.0001840959729624,7.4821503512398477E-5,0.10835680732960457,0]
["0VLPc","Basis-He","MBWR",290.00124702634298,0.41599999999999993,1,4.0029802322387695,null,149.1,"Helium:1",1505.9861165584591,31.289130846628588,5.1925512161922347,6.9051041052550652E-2,null,3005.4722874438639,"Helium:1",6028.4326546095435,125.24977226298655,20.785679873304897,1.7249908080093638E-2,7773.3802679600985,1.0001840959729624,7.4821503512398477E-5,0.10835680732960457,0]
["10HPa","Basis-He","MBWR",12.150134108509008,19.375,1,4.0029802322387695,null,225.06391648406338,"Helium:1",44.310202666293158,5.7308001623019651,6.9366376258011737,84.620830037117926,null,4536.7093487352968,"Helium:1",177.37286535966513,22.940279764605499,27.76722329428577,21.139457386176389,9.5748304405337343,0.90727734927457215,3.3526042305661477E-6,3.9619136672324858E-6,0]
["10LPa","Basis-He","MBWR",10.556487412753938,1.1691002608869878,1,4.0029802322387695,null,401.16391648406335,"Helium:1",52.984224432328595,11.821851968152124,5.4370494649981396,5.4794951938199601,null,8086.4321510080299,"Helium:1",212.0948030231138,47.322639736965947,21.764401530091931,1.3688539228072609,263.56261813523548,0.97307985735454117,1.5183224446705837E-6,2.7709166464513396E-5,0]
["11HPa","Basis-He","MBWR",7.9237944138031366,19.355,1,4.0029802322387695,null,225.06391648406338,"Helium:1",17.463045441354716,3.0476654919349042,5.1005421647293216,131.50522170703695,null,4536.7093487352968,"Helium:1",69.904225696430288,12.199744718691667,20.417369459111818,32.851828906856547,6.1612009684880231,0.89428035123414529,5.0568879052856537E-6,3.8453894375017469E-6,0]
["11LPa","Basis-He","MBWR",7.8310111137867011,1.1708187625208664,1,4.0029802322387695,null,66.563916484063455,"Helium:1",37.899942480226692,10.164334110009642,5.6735387682335103,7.6915449725193481,null,1341.7572524250863,"Helium:1",151.71272055133386,40.687628516238846,22.711063536079038,1.9214546478581169,31.155002044295138,0.9358687791458522,1.3080166934866207E-6,1.7005903211382809E-5,0]
["11LPb","Basis-He","MBWR",7.831011113783461,1.1708187625208664,1,4.0029802322387695,null,401.16391648406335,"Helium:1",37.899942480226692,10.164322718217598,5.6735411489025003,7.6915633252790867,null,8086.4321510080299,"Helium:1",151.71272055133386,40.68758291512048,22.711073065849945,1.9214592326321287,187.76288229938299,0.9358665460794201,1.3080168522266984E-6,1.7005864697593673E-5,0]
["12HPa","Basis-He","MBWR",6.9888849295174964,19.344999999999999,1,4.0029802322387695,null,225.06391648406338,"Helium:1",13.030163380304787,2.4534327316571849,4.3842007236298626,141.25990423693096,null,4536.7093487352968,"Helium:1",52.159486434201568,9.8210427259512763,17.54986883085725,35.288683940846674,5.7357401147862435,0.94340602715944011,5.7466763826242367E-6,4.0681582036085131E-6,0]
["12HPb","Basis-He","MBWR",7.0012139381660745,19.195,1,4.0029802322387695,null,225.06391648406338,"Helium:1",13.030163380304787,2.4686305301016511,4.4076879819684844,140.85968360428612,null,4536.7093487352968,"Helium:1",52.159486434201568,9.8818792126980242,17.643887861696236,35.188703274087047,5.7520369108508653,0.93709747805061872,5.7125554882604953E-6,4.0554936246404231E-6,0]
["12LPa","Basis-He","MBWR",5.3348967307537123,1.1717734856507986,1,4.0029802322387695,null,66.563916484063398,"Helium:1",22.836228684848166,7.8342394159391242,6.7476218380623845,12.945462357277592,null,1341.7572524250863,"Helium:1",91.412972004331166,31.360305516630117,27.010596832386355,3.233956104259228,18.5107408858143,0.81687723543250057,1.0982188550960303E-6,8.4834270479234077E-6,0]
["12MPa","Basis-He","MBWR",5.4348734949182358,3.0100000000000002,1,4.0029802322387695,null,225.06391648406338,"Helium:1",3.8534687226967939,3.1074954305039482,19.304769338964761,94.684422874108407,null,4536.7093487352968,"Helium:1",15.425359122505647,12.43924278007961,77.276610051805037,23.653482500750126,8.5571636257413015,0.28161464077841142,2.6076264591921869E-6,2.7540184330629173E-6,0]
["12MPb","Basis-He","MBWR",5.4348734949182358,3.0100000000000002,1,4.0029802322387695,null,66.563916484063398,"Helium:1",3.8534687226967939,3.1074954305039482,19.304769338964761,94.684422874108407,null,1341.7572524250863,"Helium:1",15.425359122505647,12.43924278007961,77.276610051805037,23.653482500750126,2.5308291698755809,0.28161464077841142,2.6076264591921869E-6,2.7540184330629173E-6,0]
["13LPa","Basis-He","MBWR",4.3999999999999773,1.1927282087807312,3.5031203732923705E-2,4.0029802322387695,null,66.563916484063398,"Helium:1",-3.562583608600931,1.964545024686086,6.2435712415796267,103.02996403657311,null,1341.7572524250863,"Helium:1",-14.260951760927389,7.8640348991614282,24.992892258617715,25.738314470504129,2.3258292049637665,null,"---","---","---"]
["13LPb","Basis-He","MBWR",4.4003144185588212,1.1927282087807312,1,4.0029802322387695,null,66.563916484063398,"Helium:1",15.345060581160505,6.2529447632887898,10.280763697383284,20.033064219146901,null,1341.7572524250863,"Helium:1",61.425974168891862,25.030414280725957,41.153693852943249,5.0045373838738385,11.961729704515108,0.65142902926256274,1.0352456699193817E-6,5.1676850760051476E-6,0]
["13LPc","Basis-He","MBWR",4.400314407842643,1.1927282087807312,1,4.0029802322387695,null,66.563916484063398,"Helium:1",15.345060581160505,6.2526353682955031,10.28238092501846,20.034966767583498,null,1341.7572524250863,"Helium:1",61.425974168891862,25.029175778683879,41.160167583197889,5.0050126668695611,11.960593801949742,0.651367170238072,1.0352588127245994E-6,5.1672599447464224E-6,0]
["13LPd","Basis-He","MBWR",4.3831043620451169,1.1727282087807311,0.99806695588048266,4.0029802322387695,null,66.563916484063398,"Helium:1",15.345060581160505,6.2758991253299579,10.10645817066311,19.674141121190871,null,1341.7572524250863,"Helium:1",61.425974168891862,25.122300138220407,40.455952275112423,4.9148734142480643,12.179952246277447,null,"---","---","---"]
["13MPa","Basis-He","MBWR",4.4850000000000136,3,0,4.0029802322387695,null,66.563916484063398,"Helium:1",-3.562583608718831,1.6401825448503515,4.6075418284584675,129.84409328259358,null,1341.7572524250863,"Helium:1",-14.260951760927389,6.5656183042990364,18.443898858532521,32.436855979669659,1.84552175832208,0.24802377839778314,1.4390502433437569E-3,1.1082908794409294E-3,0]
["1HPa","Basis-He","MBWR",156.43316311985058,19.690000000000001,1,4.0029802322387686,null,783.94203914135699,"Helium:1",818.58356328431319,20.074432884357428,5.1978222797648117,5.9505537331920992,null,15802.254014765809,"Helium:1",3276.773822262679,80.357558009486681,20.806779836588795,1.4865308814837939,474.27373442016744,1.0183949050424193,1.2278726260939915E-5,2.0634594378081761E-4,0]
["1HPb","Basis-He","MBWR",156.43316311985058,19.690000000000001,1,4.0029802322387695,null,609.30799242453509,"Helium:1",818.58356328431296,20.074432884357424,5.1978222797648117,5.9505537331921001,null,12282.08105801473,"Helium:1",3276.7738222626786,80.357558009486681,20.806779836588795,1.4865308814837939,368.62263094827074,1.0183949050424193,1.2278726260939915E-5,2.0634594378081761E-4,0]
["1LPa","Basis-He","MBWR",150.70739007286363,1.096541303012122,1,4.0029802322387695,null,401.16391648406335,"Helium:1",782.90760472689351,25.877327757395712,5.1929145295159023,0.34993376199322096,null,8086.4321510080299,"Helium:1",3133.9636653911589,103.58643147601865,20.787134209357646,8.741830878278195E-2,4127.0384747002654,1.0010627700369803,1.161784506959259E-5,3.3200126227939265E-3,0]
["1MPa","Basis-He","MBWR",150.70737349512612,5.12,1,4.0029802322387695,null,368.35255834067618,"Helium:1",784.18964262597603,22.676944555366045,5.1941489747470309,1.627579738316755,null,7425.0396116831089,"Helium:1",3139.0956377581674,90.77536078270488,20.792075669215635,0.40659199993263251,814.74915102952605,1.00496258948057,1.162618538447295E-5,7.1432355114575013E-4,0]
["2HPa","Basis-He","MBWR",135.23484061663902,19.670000000000002,1,4.0029802322387695,null,609.30799242453509,"Helium:1",708.35195610538688,19.319416605308263,5.2019936004822558,6.8562642416424797,null,12282.08105801473,"Helium:1",2835.5188777575281,77.335242769434416,20.823477550963052,1.7127899324668756,319.92768881422973,1.0213743080674464,1.0365951478222474E-5,1.5118949785020562E-4,0]
["2K Return","Basis-He","MBWR",3.8999999999999773,2.6999999999999996E-2,1,4.0029802322387695,null,149.1,"Helium:1",20.102131460350371,14.573435420728586,5.2465034204780414,0.33593747711453104,null,3005.4722874438639,"Helium:1",80.468434861647609,58.337173904984823,21.001649480546689,8.3921842633394514E-2,1597.7973181509683,0.99219586026926221,8.5616242200566878E-7,2.5485766856365885E-4,0]
["2LPa","Basis-He","MBWR",133.89598299229343,1.100742084783825,1,4.0029802322387695,null,401.16391648406335,"Helium:1",695.6072729330474,25.255017151312945,5.1931193367524981,0.39533403635247177,null,8086.4321510080299,"Helium:1",2784.5021629525072,101.0953344215568,20.787954048677161,9.8759927208376716E-2,3653.0881900970894,1.0011762220615676,1.0225049521931367E-5,2.5864328850286294E-3,0]
["2MPa","Basis-He","MBWR",133.89597068421381,5.14,1,4.0029802322387695,null,368.35255834067618,"Helium:1",696.86771277692321,22.054416940167673,5.1951042974449368,1.8378740963329103,null,7425.0396116831089,"Helium:1",2789.5476787314683,88.283395045043051,20.795899807090763,0.45912644822256143,721.5234235426276,1.0056261640882338,1.0234562753442926E-5,5.5686963398982753E-4,0]
["3HPa","Basis-He","MBWR",63.564068998623156,19.650000000000002,1,4.0029802322387695,null,609.30799242453509,"Helium:1",333.95002795718318,15.374568089307072,5.2732797203718436,14.285271889592059,null,12282.08105801473,"Helium:1",1336.7953604681886,61.544092140705196,21.108834479714076,3.5686591141627129,153.55036919713581,1.0418832679195718,6.2970883472331285E-6,4.4080983518563986E-5,0]
["3LPa","Basis-He","MBWR",60.544981859495863,1.1284290555518657,1,4.0029802322387695,null,401.16391648406335,"Helium:1",314.58814182192646,21.080512023970449,5.198121794277208,0.89510800026515069,null,8086.4321510080299,"Helium:1",1259.2901130098981,84.384872917425398,20.807978787261188,0.22361039733752033,1613.4255295616028,1.0024838338468034,5.9325949302952797E-6,6.6277979065519632E-4,0]
["3MPa","Basis-He","MBWR",60.544972850749275,5.16,1,4.0029802322387695,null,368.35255834067618,"Helium:1",315.32369065672253,17.916887615551673,5.2176053303241403,4.0571309805613565,null,7425.0396116831089,"Helium:1",1262.2345004554331,71.720946948296969,20.885970996911169,1.0135276082271087,326.84900151854492,1.0113681996783903,5.9558722111656408E-6,1.4680009690842095E-4,0]
["4HPa","Basis-He","MBWR",50.532970619770879,19.63,1,4.0029802322387695,null,609.30799242453509,"Helium:1",264.90652513999748,14.160826544793471,5.3293676848323139,17.840878767957498,null,12282.08105801473,"Helium:1",1060.4155835264726,56.685508730970298,21.333353492715851,4.4568990434358273,122.94847138740177,1.0483008503174536,5.2405702836672605E-6,2.9373947056236983E-5,0]
["4HPb","Basis-He","MBWR",50.538364113000625,19.54,1,4.0029802322387695,null,609.30799242453509,"Helium:1",264.92293720109683,14.17115441568582,5.3287716052361329,17.761035795502497,null,12282.08105801473,"Helium:1",1060.4812806826235,56.726850993993487,21.330967397875497,4.4369531611624229,123.50117402971357,1.0480736435834135,5.2400693631325064E-6,2.9503174383891579E-5,0]
["4LPa","Basis-He","MBWR",50.046423415195676,1.1343483389574469,1,4.0029802322387695,null,401.16391648406335,"Helium:1",260.00092577659132,20.079436232545305,5.2013862343617703,1.0882387435153618,null,8086.4321510080299,"Helium:1",1040.7785662474746,80.377586313377762,20.821046276389019,0.27185713652818522,1327.0893983037479,1.0027805916941794,5.0330876154448217E-6,4.6249847705167409E-4,0]
["4LPb","Basis-He","MBWR",50.046423415195676,1.1343483389574469,1,4.0029802322387695,null,401.16391648406335,"Helium:1",260.00092577659132,20.079436232545305,5.2013862343617703,1.0882387435153618,null,8086.4321510080299,"Helium:1",1040.7785662474746,80.377586313377762,20.821046276389019,0.27185713652818522,1327.0893983037479,1.0027805916941794,5.0330876154448217E-6,4.6249847705167409E-4,0]
["4MPa","Basis-He","MBWR",50.046559539717123,5.18,1,4.0029802322387695,null,194.31851162385408,"Helium:1",260.48169650086498,16.913921442215813,5.2321110918149403,4.9206283806228353,null,3916.9611108171152,"Helium:1",1042.7030819529812,67.706093182829363,20.944037273412413,1.2292412390632386,142.16611939252533,1.0127253364093272,5.0624089765471388E-6,1.0288135142419264E-4,0]
["4MPb","Basis-He","MBWR",50.046495225510796,5.18,1,4.0029802322387695,null,368.35255834067618,"Helium:1",260.48136000218454,16.913914718490155,5.2321112100431204,4.9206346666670022,null,7425.0396116831089,"Helium:1",1042.7017349554153,67.70606626788846,20.944037746677481,1.2292428094042849,269.49149852749565,1.0127253441070663,5.0624031299466921E-6,1.0288110117664391E-4,0]
["5HPa","Basis-He","MBWR",50.538570176605191,19.52,1,4.0029802322387695,null,609.30799242453509,"Helium:1",264.92129599498691,14.173350813791432,5.3286450591603769,17.743630496943595,null,12282.08105801473,"Helium:1",1060.4747109670084,56.735643132192379,21.330460836435776,4.4326050760985183,123.62232030847159,1.0480236604794106,5.2398744046346305E-6,2.9531016245729519E-5,0]
["5HPb","Basis-He","MBWR",50.538570176605191,19.52,1,4.0029802322387695,null,571.45322654407516,"Helium:1",264.92129599498685,14.173350813791432,5.3286450591603769,17.743630496943595,null,11519.026398045597,"Helium:1",1060.4747109670081,56.735643132192379,21.330460836435776,4.4326050760985183,115.94197793473192,1.0480236604794106,5.2398744046346305E-6,2.9531016245729519E-5,0]
["5LPa","Basis-He","MBWR",50.045996815185021,1.1343483389574469,1,4.0029802322387695,null,401.16391648406335,"Helium:1",259.99870686839699,20.0793918952902,5.2013864108832104,1.0882480080102042,null,8086.4321510080299,"Helium:1",1040.7696840018355,80.377408832222031,20.821046983000855,0.27185945092753394,1327.0781004995752,1.0027806025902304,5.0330498154846823E-6,4.6249106623106164E-4,0]
["5MPa","Basis-He","MBWR",50.045991911919884,5.2,1,4.0029802322387695,null,194.31851162385408,"Helium:1",260.48113117079151,16.905804087972161,5.2322613209755557,4.9394425213714541,null,3916.9611108171152,"Helium:1",1042.7008189478724,67.673599574253942,20.944638637772663,1.2339412724526355,141.6246142796785,1.0127746355141867,5.0625164813236278E-6,1.0249165689082666E-4,0]
["6HPa","Basis-He","MBWR",35.448082919989048,19.5,1,4.0029802322387695,null,571.45322654407516,"Helium:1",183.54087261008829,12.261476194795749,5.4832249337659471,25.139905130880305,null,11519.026398045597,"Helium:1",734.71048486603763,49.082446825833635,21.949241018783823,6.2802970967508793,81.831319762288786,1.0535009555824761,3.977735382368654E-6,1.5822396153287981E-5,0]
["6HPb","Basis-He","MBWR",35.448082919989048,19.5,1,4.0029802322387695,null,414.689480800681,"Helium:1",183.54087261008829,12.261476194795749,5.4832249337659471,25.139905130880305,null,8359.0727192550712,"Helium:1",734.71048486603763,49.082446825833635,21.949241018783823,6.2802970967508793,59.382965970252911,1.0535009555824761,3.977735382368654E-6,1.5822396153287981E-5,0]
["6LPa","Basis-He","MBWR",35.051685990578648,1.1559250816939202,1,4.0029802322387695,null,401.16391648406335,"Helium:1",181.93906677169772,18.186079396171145,5.2127150150207644,1.5830130038228958,null,8086.4321510080299,"Helium:1",728.29848775907556,72.798516324797873,20.866395161422339,0.3954586113300777,912.30463417229214,1.0029816843953983,3.6807597306406566E-6,2.3251607673163829E-4,0]
["6MPa","Basis-He","MBWR",35.05168686782477,5.22,1,4.0029802322387695,null,194.31851162385408,"Helium:1",181.72695354556393,15.026775879666873,5.2812275280422281,7.0735375202537867,null,3916.9611108171152,"Helium:1",727.4494027078656,60.151886800588841,21.140649396708262,1.7670678119481318,98.896293381190134,1.0136350703543349,3.7264109624731227E-6,5.2681009350741738E-5,0]
["7HPa","Basis-He","MBWR",35.296250494304672,19.48,1,4.0029802322387695,null,414.689480800681,"Helium:1",182.70813009858719,12.240047692438528,5.4855741327631327,25.224116880844527,null,8359.0727192550712,"Helium:1",731.37703305395394,48.996668954491199,21.958644815931152,6.3013343602592036,59.184713499966499,1.0534189324630201,3.965447009867288E-6,1.5720855673955003E-5,0]
["7LPa","Basis-He","MBWR",34.939378858739616,1.1568798048238527,1,4.0029802322387695,null,401.16391648406335,"Helium:1",181.35357775584001,18.167629748174253,5.2128740304721237,1.5894136266755874,null,8086.4321510080299,"Helium:1",725.95478680240421,72.724662748574545,20.867031697130752,0.39705757572194328,908.63075231290918,1.0029813041162119,3.6707989877055229E-6,2.3095303362809054E-4,0]
["8HPa","Basis-He","MBWR",21.466215437194109,19.46,1,4.0029802322387695,null,414.689480800681,"Helium:1",104.23056939328964,9.410660254151896,5.9756591330324786,42.350720646222804,null,8359.0727192550712,"Helium:1",417.23290887632976,37.670686969685114,23.920445384126076,10.579797598085333,35.250454020682632,1.0305836719242436,3.1177455683882273E-6,7.3617296726361491E-6,0]
["8HPb","Basis-He","MBWR",22.101261045659498,19.46,1,4.0029802322387686,null,560.36391648406322,"Helium:1",108.0118468528748,9.584253304139688,5.9335334844757472,41.010169108346403,null,11295.494445850842,"Helium:1",432.36928779965899,38.365576517240271,23.751817245683238,10.244909224897777,49.190484779836332,1.0336914676288258,3.1397083926362151E-6,7.6559264711669305E-6,0]
["8HPc","Basis-He","MBWR",22.100944510762588,19.414999999999999,1,4.0029802322387686,null,560.36391648406334,"Helium:1",108.02076962583163,9.5896267986062416,5.9324207456316227,40.921483260104004,null,11295.494445850843,"Helium:1",432.40500548342197,38.387086509367933,23.747362974086563,10.222754269565209,49.297091371792597,1.0335509812545653,3.1376149057529763E-6,7.6674026838415257E-6,0]
["8HPd","Basis-He","MBWR",22.100944510762588,19.414999999999999,1,4.0029802322387695,null,225.06391648406338,"Helium:1",108.02076962583162,9.5896267986062398,5.9324207456316218,40.921483260104011,null,4536.7093487352968,"Helium:1",432.40500548342209,38.387086509367933,23.747362974086563,10.222754269565209,19.799626865738606,1.0335509812545653,3.1376149057529763E-6,7.6674026838415257E-6,0]
["8LPa","Basis-He","MBWR",19.413272047098701,1.1637538113593662,1,4.0029802322387695,null,401.16391648406335,"Helium:1",100.13784608079624,15.079912171646312,5.2629295083724132,2.8890053627320595,null,8086.4321510080299,"Helium:1",400.84981836039589,60.364590326996996,21.067402785680876,0.72171362213205559,499.89180289263777,0.99901207531283653,2.3575784071367626E-6,8.1605193176493806E-5,0]
["9HPa","Basis-He","MBWR",14.475098012905278,19.395,1,4.0029802322387695,null,225.06391648406338,"Helium:1",60.213002091960611,6.9270214767568943,6.7093234172933123,67.504363746550879,null,4536.7093487352968,"Helium:1",241.03145709787,27.728730039751255,26.857289011121797,16.863526630207048,12.002632931771418,0.95563738789331654,3.0985173668709389E-6,4.5900993578793002E-6,0]
["9LPa","Basis-He","MBWR",14.335697125730405,1.166427036123177,1,4.0029802322387695,null,401.16391648406335,"Helium:1",73.283976734945909,13.471141184417247,5.3226966723841533,3.9527028948485192,null,8086.4321510080299,"Helium:1",293.35431020983435,53.924711866919807,21.306649561756846,0.98744002356411054,365.36773386758034,0.99106308201425608,1.9091683316145489E-6,4.8300324674104166E-5,0]
["CC1","Basis-He","MBWR",6.9628598880015602,8.1000000000000003E-2,1,4.0029802322387695,null,149.1,"Helium:1",35.940289027112129,15.303280143511328,5.2298614593020689,0.56353152131482898,null,3005.4722874438639,"Helium:1",143.8682665164778,61.258727902887927,20.935032038933585,0.14077799255073001,952.49330285488577,0.99388436636025479,1.1727697321436595E-6,2.0811076005249163E-4,0]
["CC2","Basis-He","MBWR",12.436612471434785,0.24299999999999997,1,4.0029802322387695,null,149.1,"Helium:1",64.276900521282457,16.035807624694762,5.2280805165878688,0.94382122888950726,null,3005.4722874438639,"Helium:1",257.29916217627152,64.191020929636863,20.927902960453892,0.23577963770299484,568.70939492593061,0.99671533516571609,1.6910715891896451E-6,1.7917287060594591E-4,0]
["From Buffer","Basis-He","MBWR",300,1.05,1,4.0029802322387695,null,0,"Helium:1",1558.1098587914169,29.54223261429339,5.1925011369304093,0.16842953413554695,null,0,"Helium:1",6237.0829643983825,118.2569731712159,20.785479407009763,4.2076034445303369E-2,0,1.0004756126447814,8.5038393476688577E-5,5.0489003554597664E-2,0]
["From Subcooler","Basis-He","MBWR",4.5,3,0,4.0029802322387695,null,157.69999999999999,"Helium:1",-3.4931821888927241,1.6556308082427016,4.6461209327765491,129.56267548664505,null,3178.8261551300957,"Helium:1",-13.983139249746131,6.6274573972810309,18.59833025049528,32.366553909806292,4.381817509306674,0.24773395904823198,1.4142555626009659E-3,1.0915609432183603E-3,0]
["From TS","Basis-He","MBWR",50.551917080010952,19,1,4.0029802322387695,null,156.76374574339414,"Helium:1",264.92129599498685,14.232236775563182,5.3252891990100411,17.28738527491339,null,3159.953678790524,"Helium:1",1060.4747109670081,56.971362473121061,21.317027394591825,4.3186286896163297,32.645161526837462,1.0467509648624904,5.2354938458721116E-6,3.0285053306873458E-5,0]
["From Turbines","Basis-He","MBWR",279.8043455840895,1.1708187625208664,1,4.0029802322387695,null,30.399999999999988,"Helium:1",1453.2831715739001,28.954146840982407,5.1925031889721556,0.20134612046135467,null,612.78576484435575,"Helium:1",5817.4638076555857,115.90287744579119,20.785487621292312,5.0299054399463437E-2,543.54163740147806,1.0005727297635914,6.539264262623467E-5,3.2477726651200016E-2,0]
["From Turbines 2","Basis-He","MBWR",297.01803609830199,1.05,1,4.0029802322387695,null,30.399999999999988,"Helium:1",1542.6260302418439,29.490361548066058,5.1925023717723473,0.1701195819746455,null,612.78576484435575,"Helium:1",6175.1015047950668,118.04933431848275,20.785484350057633,4.2498231843503695E-2,643.31218505057711,1.0004810794911707,8.1888635539003381E-5,4.8135925675627404E-2,0]
["GHe Return","Basis-He","MBWR",300,1.05,1,4.0029802322387695,null,8.5999999999999979,"Helium:1",1558.1098587914169,29.54223261429339,5.1925011369304093,0.16842953413554695,null,173.35386768623226,"Helium:1",6237.0829643983825,118.2569731712159,20.785479407009763,4.2076034445303369E-2,183.81574323588839,1.0004756126447814,8.5038393476688577E-5,5.0489003554597664E-2,0]
["HPa","Basis-He","MBWR",300,19.740000000000002,1,4.0029802322387695,null,145.67443568338243,"Helium:1",1564.1474650896414,23.450900749473647,5.1911378242510127,3.1396417935258278,null,2936.4217265957709,"Helium:1",6261.2513830602156,93.873492128336352,20.780022093303778,0.78432607991419001,167.0343316048301,1.0090263366812275,8.5058331997752245E-5,2.7091731347553332E-3,0]
["HPb","Basis-He","MBWR",23.938158452081126,19.64,1,4.0029802322387695,null,145.67443568338243,"Helium:1",118.77595916347106,10.032298406446811,5.8323981107719591,37.933056246144709,null,2936.4217265957709,"Helium:1",475.45781659657399,40.159092204927092,23.346974343966899,9.4762037395647276,13.825091367729602,1.0413329749777065,3.2202128954589529E-6,8.4891996958094724E-6,0]
["HPc","Basis-He","MBWR",23.93215201849344,19.46,1,4.0029802322387695,null,145.67443568338243,"Helium:1",118.77595916347106,10.052204496220519,5.8285709823812279,37.615679591246185,null,2936.4217265957709,"Helium:1",475.45781659657399,40.238775888792418,23.331654424672561,9.3969186478367011,13.941738502638142,1.0407558974722897,3.2121885218329067E-6,8.5394935216867343E-6,0]
["HP-LPa","Basis-He","MBWR",299.99564396960591,19.809999999999999,1,4.0029802322387695,null,29.617004376022859,"Helium:1",1564.1474650896412,23.443481687159732,5.1911329756221605,3.1507205335984461,null,597.0025881236777,"Helium:1",6261.2513830602147,93.843793768552004,20.780002684338331,0.78709370289253833,33.840264351186335,1.009058519407718,8.5053747578708384E-5,2.6995014845562419E-3,0]
["HP-LPb","Basis-He","MBWR",301.16275679975115,1.05,1,4.0029802322387695,null,29.617004376022859,"Helium:1",1564.1474650896412,29.562303722551412,5.1925006766621324,0.16778009488432205,null,597.0025881236777,"Helium:1",6261.2513830602147,118.3373174208119,20.78547756456495,4.1913795509923545E-2,635.48191355591689,1.0004705503669673,8.6290641284415357E-5,5.143079776174251E-2,0]
["LevelCompensation","Basis-He","MBWR",4.4003144185588212,1.1927282087807312,1,4.0029802322387695,null,0,"Helium:1",15.345060581160505,6.2529447632887898,10.280763697383284,20.033064219146901,null,0,"Helium:1",61.425974168891862,25.030414280725957,41.153693852943249,5.0045373838738385,0,0.65142902926256274,1.0352456699193817E-6,5.1676850760051476E-6,0]
["LHe","Basis-He","MBWR",4.4003144185588212,1.1927282087807312,0,4.0029802322387695,null,0,"Helium:1",-4.2469505978300788,1.809326236110294,6.0993858239616836,121.25339758093016,null,0,"Helium:1",-17.000459290408429,7.2426971568204834,24.415720882115998,30.290781004710603,0,0.10762683634265333,1.5084733513140631E-3,1.2440668726888563E-3,0]
["LP-VLPa","Basis-He","MBWR",297.01679104003063,1.07,1,4.0029802322387695,null,0,"Helium:1",1542.6260302436067,29.451151908754547,5.1925008740433043,0.17335908042110304,null,0,"Helium:1",6175.1015048021236,117.89237890740556,20.785478354677881,4.3307503500747371E-2,0,1.000490320528387,8.188738430893805E-5,4.723570528294628E-2,0]
["LP-VLPb","Basis-He","MBWR",297.05750396914084,0.41599999999999993,1,4.0029802322387695,null,0,"Helium:1",1542.6260302436067,31.413959248640918,5.1925499325930904,6.7411212478687338E-2,null,0,"Helium:1",6175.1015048021236,125.74945788866387,20.785674735082896,1.6840256151099173E-2,0,1.0001781770454703,8.1929041661352381E-5,0.12153622320211938,0]
["Supply 2K","Basis-He","MBWR",4.5,3,0,4.0029802322387695,null,149.1,"Helium:1",-3.4931821888927241,1.6556308082427016,4.6461209327765491,129.56267548664505,null,3005.4722874438639,"Helium:1",-13.983139249746131,6.6274573972810309,18.59833025049528,32.366553909806292,4.1428598011263489,0.24773395904823198,1.4142555626009659E-3,1.0915609432183603E-3,0]
["Supply LHe","Basis-He","MBWR",4.5,3,0,4.0029802322387695,null,8.6,"Helium:1",-3.4931821888927241,1.6556308082427016,4.6461209327765491,129.56267548664505,null,173.35386768623226,"Helium:1",-13.983139249746131,6.6274573972810309,18.59833025049528,32.366553909806292,0.23895770818032591,0.24773395904823198,1.4142555626009659E-3,1.0915609432183603E-3,0]
["T1_Loss","Basis-He","MBWR",135.23484061663902,12,1,4.0029802322387695,null,0.3,"Helium:1",705.96415190651351,20.345521428864615,5.198292483269463,4.2171642631495612,null,6.0472279425429853,"Helium:1",2825.9605447509816,81.442720094335343,20.808662051923044,1.0535061425449517,0.25609626104376809,1.0130452507002556,1.0344034245635066E-5,2.4528411985331804E-4,0]
["T1Ha","Basis-He","MBWR",156.43316311985058,19.690000000000001,1,4.0029802322387695,null,174.63404671682213,"Helium:1",818.58356328431296,20.074432884357424,5.1978222797648117,5.9505537331921001,null,3520.1729567510806,"Helium:1",3276.7738222626786,80.357558009486681,20.806779836588795,1.4865308814837939,105.65110347189669,1.0183949050424193,1.2278726260939915E-5,2.0634594378081761E-4,0]
["T1Hb","Basis-He","MBWR",156.44236285742156,19.54,1,4.0029802322387695,null,174.63404671682216,"Helium:1",818.58356328431296,20.09065218536659,5.1977795312202053,5.9056442637220687,null,3520.1729567510806,"Helium:1",3276.7738222626786,80.422483550807101,20.80660871500978,1.4753118729290315,106.45452724650377,1.0182621938830108,1.2279415280122146E-5,2.0792676855857503E-4,0]
["T1La","Basis-He","MBWR",135.23484061663902,12,1,4.0029802322387695,null,174.63404671682216,"Helium:1",705.96415190651351,20.345521428864615,5.198292483269463,4.2171642631495612,null,3520.1729567510806,"Helium:1",2825.9605447509816,81.442720094335343,20.808662051923044,1.0535061425449517,149.07708805040292,1.0130452507002556,1.0344034245635066E-5,2.4528411985331804E-4,0]
["T1Lb","Basis-He","MBWR",135.23484061663902,12,1,4.0029802322387695,null,174.33404671682214,"Helium:1",705.96415190651351,20.345521428864615,5.198292483269463,4.2171642631495612,null,3514.1257288085376,"Helium:1",2825.9605447509816,81.442720094335343,20.808662051923044,1.0535061425449517,148.82099178935917,1.0130452507002556,1.0344034245635066E-5,2.4528411985331804E-4,0]
["T2_Loss","Basis-He","MBWR",50.046423415195676,5.18,1,4.0029802322387695,null,0.3,"Helium:1",260.48098428304235,16.913907628144877,5.2321113347181845,4.9206412954743071,null,6.0472279425429862,"Helium:1",1042.7002309591162,67.706037885376475,20.944038245749297,1.2292444653723189,0.21948358661975934,1.0127254329526192,5.0623965851170581E-6,1.0288082957343648E-4,0]
["T2Ha","Basis-He","MBWR",63.564068998623156,11.98,1,4.0029802322387695,null,174.33404671682214,"Helium:1",332.41846487448942,16.41193635736731,5.243079498863362,8.8486443978527944,null,3514.1257288085376,"Helium:1",1330.6645437237387,65.696656811302105,20.987943590006392,2.2105141380885516,70.92640860704644,1.0254750424744594,6.2403775700292533E-6,7.0523543375113366E-5,0]
["T2Hb","Basis-He","MBWR",63.569745412009922,11.83,1,4.0029802322387695,null,174.33404671682214,"Helium:1",332.41846487448942,16.439056120610562,5.2424537979691523,8.7393415863613146,null,3514.1257288085376,"Helium:1",1330.6645437237389,65.805216687467833,20.985438921695575,2.183208779293325,71.813484114181009,1.0252086642995615,6.2397751977108085E-6,7.1398687601920155E-5,0]
["T2La","Basis-He","MBWR",50.046423415195676,5.18,1,4.0029802322387695,null,174.33404671682214,"Helium:1",260.4809842830424,16.913907628144877,5.2321113347181845,4.9206412954743071,null,3514.1257288085376,"Helium:1",1042.7002309591164,67.706037885376475,20.944038245749297,1.2292444653723189,127.54487281114936,1.0127254329526192,5.0623965851170581E-6,1.0288082957343648E-4,0]
["T2Lb","Basis-He","MBWR",50.046423415195676,5.18,1,4.0029802322387695,null,174.03404671682216,"Helium:1",260.48098428304235,16.913907628144877,5.2321113347181845,4.9206412954743071,null,3508.0785008659946,"Helium:1",1042.7002309591162,67.706037885376475,20.944038245749297,1.2292444653723189,127.3253892245296,1.0127254329526192,5.0623965851170581E-6,1.0288082957343648E-4,0]
["T3_Loss","Basis-He","MBWR",34.939378858739616,5.24,1,4.0029802322387695,null,0.3,"Helium:1",181.13282385295346,15.001747271684524,5.2821792999718689,7.1231677172556278,null,6.0472279425428912,"Helium:1",725.07111329295981,60.051697777595045,21.144459320928213,1.7794661237364675,0.15161793781490226,1.0136771266446278,3.716875084631387E-6,5.2180086615500937E-5,0]
["T3Ha","Basis-He","MBWR",50.538570176605191,19.52,1,4.0029802322387695,null,37.854765880459922,"Helium:1",264.92129599498685,14.173350813791432,5.3286450591603769,17.743630496943595,null,763.05465996913381,"Helium:1",1060.4747109670081,56.735643132192379,21.330460836435776,4.4326050760985183,7.6803423737396903,1.0480236604794106,5.2398744046346305E-6,2.9531016245729519E-5,0]
["T3Hb","Basis-He","MBWR",50.551917080010952,19,1,4.0029802322387695,null,37.854765880459922,"Helium:1",264.92129599498685,14.232236775563182,5.3252891990100411,17.28738527491339,null,763.05465996913381,"Helium:1",1060.4747109670081,56.971362473121061,21.317027394591825,4.3186286896163297,7.8830404368562617,1.0467509648624904,5.2354938458721116E-6,3.0285053306873458E-5,0]
["T3Hc","Basis-He","MBWR",50.551917078098398,19,1,4.0029802322387695,null,194.61851162385406,"Helium:1",264.92129599498685,14.232079214296729,5.3252979811839953,17.28788470052303,null,3923.0083387596578,"Helium:1",1060.4747109670081,56.970731758486082,21.317062549460559,4.3187534530627287,40.527031154058875,1.046720725561199,5.2354999080688242E-6,3.0284213475292494E-5,0]
["T3La","Basis-He","MBWR",34.939378858739616,5.24,1,4.0029802322387695,null,194.61851162385406,"Helium:1",181.13282385295346,15.001747271684524,5.2821792999718689,7.1231677172556278,null,3923.0083387596578,"Helium:1",725.07111329295981,60.051697777595045,21.144459320928213,1.7794661237364675,98.35885797671601,1.0136771266446278,3.716875084631387E-6,5.2180086615500937E-5,0]
["T3Lb","Basis-He","MBWR",34.939378858739616,5.24,1,4.0029802322387695,null,194.31851162385408,"Helium:1",181.13282385295346,15.001747271684524,5.2821792999718689,7.1231677172556278,null,3916.9611108171152,"Helium:1",725.07111329295981,60.051697777595045,21.144459320928213,1.7794661237364675,98.207240038901105,1.0136771266446278,3.716875084631387E-6,5.2180086615500937E-5,0]
["T4_Loss","Basis-He","MBWR",14.475098012905278,4.8239999999999998,1,4.0029802322387695,null,0.3,"Helium:1",70.544177845277019,10.387001255035749,5.7318436578659,16.583770271199473,null,6.0472279425429862,"Helium:1",282.38694941418004,41.578960696147391,22.944456856720358,4.1428558996217113,6.5123912255080074E-2,0.96751837749372294,2.0563483838942173E-6,1.239976404801877E-5,0]
["T4Ha","Basis-He","MBWR",22.100944510762588,19.414999999999999,1,4.0029802322387695,null,335.3,"Helium:1",108.02076962583162,9.5896267986062398,5.9324207456316218,40.921483260104011,null,6758.7850971155449,"Helium:1",432.40500548342209,38.387086509367933,23.747362974086563,10.222754269565209,29.49746450605398,1.0335509812545653,3.1376149057529763E-6,7.6674026838415257E-6,0]
["T4Hb","Basis-He","MBWR",22.094840730879525,19.265000000000001,1,4.0029802322387695,null,335.30000000000007,"Helium:1",108.02076962583162,9.6062960215679336,5.9290025706776204,40.635592152541925,null,6758.7850971155449,"Helium:1",432.40500548342209,38.453813079370377,23.733680087315363,10.151334704397335,29.704993481299429,1.033066444234626,3.1304402576464712E-6,7.7036905132208065E-6,0]
["T4La","Basis-He","MBWR",14.475098012905278,4.8239999999999998,1,4.0029802322387695,null,335.30000000000007,"Helium:1",70.544177845277019,10.387001255035749,5.7318436578659,16.583770271199473,null,6758.7850971155449,"Helium:1",282.38694941418004,41.578960696147391,22.944456856720358,4.1428558996217113,72.786825930427824,0.96751837749372294,2.0563483838942173E-6,1.239976404801877E-5,0]
["T4Lb","Basis-He","MBWR",14.475098012905278,4.8239999999999998,1,4.0029802322387695,null,335,"Helium:1",70.544177845277019,10.387001255035749,5.7318436578659,16.583770271199473,null,6752.7378691730009,"Helium:1",282.38694941418004,41.578960696147391,22.944456856720358,4.1428558996217113,72.721702018172749,0.96751837749372294,2.0563483838942173E-6,1.239976404801877E-5,0]
["T5_Loss","Basis-He","MBWR",7.8310111137867011,1.1708187625208664,1,4.0029802322387695,null,0.4,"Helium:1",37.899942480226692,10.164334110009642,5.6735387682335103,7.6915449725193481,null,8.062970590057315,"Helium:1",151.71272055133386,40.687628516238846,22.711063536079038,1.9214546478581169,0.18721856338939549,0.9358687791458522,1.3080166934866207E-6,1.7005903211382809E-5,0]
["T5Ha","Basis-He","MBWR",12.150134108509008,4.8040000000000003,1,4.0029802322387695,null,334.99999999999994,"Helium:1",56.961264911342504,9.3716217051300585,6.0017974523824096,20.376850122446367,null,6752.7378691730009,"Helium:1",228.0148174434199,37.514416429655412,24.025076559787792,5.090419872258547,59.184809857904185,0.93420370642106132,1.8663437859793204E-6,9.1591378194583026E-6,0]
["T5Hb","Basis-He","MBWR",12.118419549907571,4.6539999999999999,1,4.0029802322387695,null,334.99999999999994,"Helium:1",56.961264911342504,9.4332135426035642,5.9796491671824459,19.765870927977655,null,6752.7378691730009,"Helium:1",228.0148174434199,37.760967337529124,23.936417411954352,4.9377887926573854,61.014260610847366,0.93545122862026076,1.8547912335206469E-6,9.38380727203514E-6,0]
["T5La","Basis-He","MBWR",7.8310111137867011,1.1708187625208664,1,4.0029802322387695,null,334.99999999999994,"Helium:1",37.899942480226692,10.164334110009642,5.6735387682335103,7.6915449725193481,null,6752.7378691730009,"Helium:1",151.71272055133386,40.687628516238846,22.711063536079038,1.9214546478581169,156.79554683861872,0.9358687791458522,1.3080166934866207E-6,1.7005903211382809E-5,0]
["T5Lb","Basis-He","MBWR",7.8310111137867011,1.1708187625208664,1,4.0029802322387695,null,334.59999999999997,"Helium:1",37.899942480226692,10.164334110009642,5.6735387682335103,7.6915449725193481,null,6744.6748985829436,"Helium:1",151.71272055133386,40.687628516238846,22.711063536079038,1.9214546478581169,156.60832827522935,0.9358687791458522,1.3080166934866207E-6,1.7005903211382809E-5,0]
["T6_Loss","Basis-He","MBWR",5.4348734949182358,3.0100000000000002,1,4.0029802322387695,null,0.8,"Helium:1",3.8534687226967939,3.1074954305039482,19.304769338964761,94.684422874108407,null,16.12594118011463,"Helium:1",15.425359122505647,12.43924278007961,77.276610051805037,23.653482500750126,3.0416830061151905E-2,0.28161464077841142,2.6076264591921869E-6,2.7540184330629173E-6,0]
["To Buffer","Basis-He","MBWR",299.99564396960591,19.809999999999999,1,4.0029802322387695,null,0,"Helium:1",1564.1474650896412,23.443481687159732,5.1911329756221605,3.1507205335984461,null,0,"Helium:1",6261.2513830602147,93.843793768552004,20.780002684338331,0.78709370289253833,0,1.009058519407718,8.5053747578708384E-5,2.6995014845562419E-3,0]
["To Subcooler","Basis-He","MBWR",5.4348734949182358,3.0100000000000002,1,4.0029802322387695,null,157.69999999999999,"Helium:1",3.8534687226967939,3.1074954305039482,19.304769338964761,94.684422874108407,null,3178.8261551300957,"Helium:1",15.425359122505647,12.43924278007961,77.276610051805037,23.653482500750126,5.9959176258045686,0.28161464077841142,2.6076264591921869E-6,2.7540184330629173E-6,0]
["To TS","Basis-He","MBWR",35.448082919989048,19.5,1,4.0029802322387695,null,156.76374574339414,"Helium:1",183.54087261008829,12.261476194795749,5.4832249337659471,25.139905130880305,null,3159.953678790524,"Helium:1",734.71048486603763,49.082446825833635,21.949241018783823,6.2802970967508793,22.448353792035871,1.0535009555824761,3.977735382368654E-6,1.5822396153287981E-5,0]
["Turbine Bearings","Basis-He","MBWR",299.99564396960591,19.809999999999999,1,4.0029802322387695,null,28,"Helium:1",1564.1474650896412,23.443481687159732,5.1911329756221605,3.1507205335984461,null,564.40794130401207,"Helium:1",6261.2513830602147,93.843793768552004,20.780002684338331,0.78709370289253833,31.992681967535873,1.009058519407718,8.5053747578708384E-5,2.6995014845562419E-3,0]
["VLPa","Basis-He","MBWR",18.103381794872718,0.48599999999999993,1,4.0029802322387695,null,149.1,"Helium:1",93.681086843906641,16.547288860092742,5.2264783134879877,1.2937715665074836,null,3005.4722874438639,"Helium:1",375.00353877080175,66.238470204096046,20.921489373117037,0.32320208730681355,414.88004056927554,0.99902341248339854,2.2326581121300741E-6,1.7256973100414474E-4,0]

{"sheet":"AUX","index":13,"n_rows":34,"n_cols":23,"rows_kept":34,"cut":false,"hidden":false,"merged":[]}
["YES","--------",1,"msoLineSolid","X","K",null,"Temperature","Pressure","Mass Flow","Mass Enthalpy","Mass Entropy","Mass Heat capacity","Mass Density","Molar Flow","Molar Enthalpy","Molar Entropy","Molar Heat capacity","Molar Density","Volume Flow","Dynamic Viscosity","Kinematic viscosity","Thermal conductivity"]
["NO",". . . . . (carré)",2,"msoLineSquareDot",null,"bar",null,"C","kPa","kg/h","kJ/g","kJ/g-C","kJ/g-C","kg/m3","kgmole/h","kJ/gmole","kJ/gmole-C","kJ/gmole-C","kgmole/m3","m3/h","cP","cSt","W/m-K"]
[null,". . . . . (rond)",3,"msoLineRoundDot",null,"g/s",null,"K","MPa","kg/min","kJ/kg","kJ/g-K","kJ/g-K","g/L","kgmole/min","kJ/kgmole","kJ/gmole-K","kJ/gmole-K","gmole/L","m3/min","mP","m²/s*","Btu/hr-ft-F"]
[null,"- - - - -",4,"msoLineDash",null,"kJ/kg",null,"F","kg/m-s2","kg/s","J/g","kJ/kg-C","kJ/kg-C","g/cm3","kgmole/s","J/gmole","kJ/kgmole-C","kJ/kgmole-C","gmole/cm3","m3/s","microP",null,"Btu/h-ft-F"]
[null,"- . - . -",5,"msoLineDashDot",null,"kJ/kg-K",null,"R","bar","kg/d","J/kg","kJ/kg-K","kJ/kg-K","g/mL","m3/h_(gas)","J/kgmole","kJ/kgmole-K","kJ/kgmole-K","gmole/mL","m3/d","P",null,"Kcal/m-hr-C"]
[null,"- . . - . .",6,"msoLineDashDotDot",null,"kJ/kg-K",null,null,"mbar","tonne/d","kcal/g","J/g-C","J/g-C","lb/ft3","m3/d_(gas)","kcal/gmole","J/gmole-C","J/gmole-C","lbmole/ft3","L/h","Pa-s",null,"cal/cm-s-C"]
[null,"-- -- --",7,"msoLineLongDash",null,"kg/m3",null,null,"N/m2","tonne/h","MJ/kg","J/g-K","J/g-K","API","Nm3/h(gas)","MJ/kgmole","J/gmole-K","J/gmole-K","Nm3/m3*","L/d","lbf-s/ft2",null,"kcal/m/°C/h*"]
[null,"-- . -- . ",8,"msoLineLongDashDot",null,"Nm3/h*",null,null,"atm","tonne/year","kcal/kg","J/kg-C","J/kg-C","SG_60/60api","Nm3/d(gas)","kcal/kgmole","J/kgmole-C","J/kgmole-C",null,"L/min","lbm/s-ft"]
[null,null,null,null,null,"J/mol*",null,null,"at","g/h","cal/g","J/kg-K","J/kg-K","SG_H2O60nbs","gmole/h","cal/gmole","J/kgmole-K","J/kgmole-K",null,"L/s","lbm/h-ft"]
[null,null,null,null,null,"kJ/kgmole-C",null,null,"kg/cm2","g/min","cal/kg","kcal/g-C","kcal/g-C","SG_H2O4","gmole/min","cal/kgmole","kcal/gmol-C","kcal/gmol-C",null,"mL/h","slug/h-ft"]
[null,null,null,null,null,"kJ/kgmole-C",null,null,"psia","g/s","Btu/lb","kcal/g-K","kcal/g-K",null,"gmole/s","Btu/lbmole","kcal/gmol-K","kcal/gmol-K",null,"mL/min","poundals/ft2"]
[null,null,null,null,null,"kgmole/m3",null,null,"lbf/ft2","lb/hr",null,"kcal/kg-C","kcal/kg-C",null,"lbmole/hr","kkcal/kgmole","kcal/kgmol-C","kcal/kgmol-C",null,"mL/s"]
[null,null,null,null,null,"m3/h",null,null,"torr","Mlb/hr",null,"kcal/kg-K","kcal/kg-K",null,"lbmole/h","Btu/SCF","kcal/kgmol-K","kcal/kgmol-K",null,"cm3/h"]
[null,null,null,null,null,"Pa-s",null,null,"mmHg(0C)","Mlb/day",null,"cal/g-C","cal/g-C",null,"MMSCFH","Btu/MSCF","cal/gmole-C","cal/gmole-C",null,"cm3/min"]
[null,null,null,null,null,"m²/s*",null,null,"inHg(32F)","MMlb/day",null,"cal/g-K","cal/g-K",null,"MMSCFD","Btu/MMSCF","cal/gmole-K","cal/gmole-K",null,"cm3/s"]
[null,null,null,null,null,"W/m-K",null,null,"inHg(60F)","lb/day",null,"cal/kg-C","cal/kg-C",null,"kscfd","kWh/Nm3*","cal/kgmole-C","cal/kgmole-C",null,"barrel/day"]
[null,null,null,null,null,null,null,null,"cmH2O(4C)","klb/day",null,"cal/kg-K","cal/kg-K",null,"MSCFD","kcal/Nm3*","cal/kgmole-K","cal/kgmole-K",null,"kbpd"]
[null,null,null,null,null,null,null,null,"inH2O(60F)","tn(short)/h",null,"Btu/lb-F","Btu/lb-F",null,"MSCFH","J/mol*","Btu/lbmole-F","Btu/lbmole-F",null,"barrel/hr"]
[null,null,null,null,null,null,null,null,"kPag","tn(short)/d",null,"Btu/lb-F","Btu/lb-F",null,"scfd",null,"Btu/lbmole-F","Btu/lbmole-F",null,"Mgal/day"]
[null,null,null,null,null,null,null,null,"MPag","tn(long)/h",null,"Btu/lb-R","Btu/lb-R",null,"Nm3/h*",null,"Btu/lbmole-R","Btu/lbmole-R",null,"MMgal/day"]
[null,null,null,null,null,null,null,null,"bar_g","tn(long)/d",null,null,null,null,null,null,"kcal/Nm3/°C*","kcal/Nm3/°C*",null,"USGPM"]
[null,null,null,null,null,null,null,null,"mbar_g","kilo ton(short)/d",null,null,null,null,null,null,"J/mol.K*","J/mol.K*",null,"USGPH"]
[null,null,null,null,null,null,null,null,"N/m2_g","kilo ton(long)/d",null,null,null,null,null,null,null,null,null,"ft3/hr"]
[null,null,null,null,null,null,null,null,"atm_g",null,null,null,null,null,null,null,null,null,null,"ft3/day"]
[null,null,null,null,null,null,null,null,"ate",null,null,null,null,null,null,null,null,null,null,"ft3/d"]
[null,null,null,null,null,null,null,null,"kg/cm2_g"]
[null,null,null,null,null,null,null,null,"psig"]
[null,null,null,null,null,null,null,null,"lbf/ft2_g"]
[null,null,null,null,null,null,null,null,"torr_g"]
[null,null,null,null,null,null,null,null,"mmHg(0C)_g"]
[null,null,null,null,null,null,null,null,"inHg(32F)_g"]
[null,null,null,null,null,null,null,null,"inHg(60F)_g"]
[null,null,null,null,null,null,null,null,"cmH2O(4C)_g"]
[null,null,null,null,null,null,null,null,"inH2O(60F)_g"]

{"sheet":"DS-HX-01","index":14,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-01"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","0HPa ~ 1HPa","1MPa ~ 0MPc","1LPa ~ 0LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",783.9420391413571,368.35255834067618,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.740000000000002,5.12,1.096541303012122]
["pressure","outlet","bar abs",19.690000000000001,5.07,1.07]
["Operating","inlet","K",300,150.70737349512612,150.70739007286363]
["temperat.","outlet","K",156.43316311985058,297.0167906089651,297.01679104003063]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-584478.88549145556,279848.2664833499,304771.61900810583,"","",""]
[null,null,null,null,null,null,"Heat leak",-139,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-02","index":15,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-02"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","1HPb ~ 2HPa","2MPa ~ 1MPa","2LPa ~ 1LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",609.30799242453509,368.35255834067618,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.690000000000001,5.14,1.100742084783825]
["pressure","outlet","bar abs",19.670000000000002,5.12,1.096541303012122]
["Operating","inlet","K",156.43316311985058,133.89597068421381,133.89598299229343]
["temperat.","outlet","K",135.23484061663902,150.70737349512612,150.70739007286363]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-67164.999271921435,32165.256259143633,35021.743012777508,"","",""]
[null,null,null,null,null,null,"Heat leak",-22,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-03","index":16,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-03"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","T1Lb ~ T2Ha","2HPa ~ 3HPa","3MPa ~ 2MPa","3LPa ~ 2LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0,0]
["fraction","outlet","%",0,0,0,0]
["Flowrate",null,"g/s",174.33404671682214,609.30799242453509,368.35255834067618,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",12,19.670000000000002,5.16,1.1284290555518657]
["pressure","outlet","bar abs",11.98,19.650000000000002,5.14,1.100742084783825]
["Operating","inlet","K",135.23484061663902,135.23484061663902,60.544972850749275,60.544981859495863]
["temperat.","outlet","K",63.564068998623156,63.564068998623156,133.89597068421381,133.89598299229343]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-65121.731253908336,-228126.08719985702,140542.7166675675,152851.12689189214,"",""]
[null,null,null,null,null,null,"Heat leak",-145,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-04","index":17,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-04"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","3HPa ~ 4HPa","4MPb ~ 3MPa","4LPb ~ 3LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",609.30799242453509,368.35255834067618,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.650000000000002,5.18,1.1343483389574469]
["pressure","outlet","bar abs",19.63,5.16,1.1284290555518657]
["Operating","inlet","K",63.564068998623156,50.046495225510796,50.046423415195676]
["temperat.","outlet","K",50.532970619770879,60.544972850749275,60.544981859495863]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-42068.758091497133,20201.312801964363,21898.421378708335,"","",""]
[null,null,null,null,null,null,"Heat leak",-31,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-05","index":18,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-05"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","4HPb ~ 5HPa","5MPa ~ 4MPa","5LPa ~ 4LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",609.30799242453509,194.31851162385408,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.54,5.2,1.1343483389574469]
["pressure","outlet","bar abs",19.52,5.18,1.1343483389574469]
["Operating","inlet","K",50.538364113000625,50.045991911919884,50.045996815185021]
["temperat.","outlet","K",50.538570176605191,50.046559539717123,50.046423415195676]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-1.0000000000047748,0.10985409844721516,0.89014590156466511,"","",""]
[null,null,null,null,null,null,"Heat leak",0,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-06","index":19,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-06"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","5HPb ~ 6HPa","6MPa ~ 5MPa","6LPa ~ 5LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",571.45322654407516,194.31851162385408,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.52,5.22,1.1559250816939202]
["pressure","outlet","bar abs",19.5,5.2,1.1343483389574469]
["Operating","inlet","K",50.538570176605191,35.05168686782477,35.051685990578648]
["temperat.","outlet","K",35.448082919989048,50.045991911919884,50.045996815185021]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-46505.105520823192,15303.394580294856,31314.710940528301,"","",""]
[null,null,null,null,null,null,"Heat leak",-113,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-07","index":20,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-07"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","6HPb ~ 7HPa","T3Lb ~ 6MPa","7LPa ~ 6LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",414.689480800681,194.31851162385408,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.5,5.24,1.1568798048238527]
["pressure","outlet","bar abs",19.48,5.22,1.1559250816939202]
["Operating","inlet","K",35.448082919989048,34.939378858739616,34.939378858739616]
["temperat.","outlet","K",35.296250494304672,35.05168686782477,35.051685990578648]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-345.32955973504897,115.45039757960751,234.87706665987673,"","",""]
[null,null,null,null,null,null,"Heat leak",-5,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-08","index":21,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-08"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","7HPa ~ 8HPa","8LPa ~ 7LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0]
["fraction","outlet","%",0,0]
["Flowrate",null,"g/s",414.689480800681,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.48,1.1637538113593662]
["pressure","outlet","bar abs",19.46,1.1568798048238527]
["Operating","inlet","K",35.296250494304672,19.413272047098701]
["temperat.","outlet","K",21.466215437194109,34.939378858739616]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-32543.818903383766,32580.820998879368,null,"","",""]
[null,null,null,null,null,null,"Heat leak",-36,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-09","index":22,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-09"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","8HPd ~ 9HPa","9LPa ~ 8LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0]
["fraction","outlet","%",0,0]
["Flowrate",null,"g/s",225.06391648406338,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.414999999999999,1.166427036123177]
["pressure","outlet","bar abs",19.395,1.1637538113593662]
["Operating","inlet","K",22.100944510762588,14.335697125730405]
["temperat.","outlet","K",14.475098012905278,19.413272047098701]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-10759.80339953266,10772.803399532648,null,"","",""]
[null,null,null,null,null,null,"Heat leak",-14,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-10","index":23,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-10"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","T4Lb ~ T5Ha","9HPa ~ 10HPa","10LPa ~ 9LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0,0]
["fraction","outlet","%",0,0,0]
["Flowrate",null,"g/s",335,225.06391648406338,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",4.8239999999999998,19.395,1.1691002608869878]
["pressure","outlet","bar abs",4.8040000000000003,19.375,1.166427036123177]
["Operating","inlet","K",14.475098012905278,14.475098012905278,10.556487412753938]
["temperat.","outlet","K",12.150134108509008,12.150134108509008,14.335697125730405]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-4550.2758328680602,-3579.1463218012309,8143.5281373743464,"","",""]
[null,null,null,null,null,null,"Heat leak",-14,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-11","index":24,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-11"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","10HPa ~ 11HPa","11LPb ~ 10LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0]
["fraction","outlet","%",0,0]
["Flowrate",null,"g/s",225.06391648406338,401.16391648406335]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.375,1.1708187625208664]
["pressure","outlet","bar abs",19.355,1.1691002608869878]
["Operating","inlet","K",12.150134108509008,7.831011113783461]
["temperat.","outlet","K",7.9237944138031366,10.556487412753938]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-6042.3263515080635,6051.2696252550704,null,"","",""]
[null,null,null,null,null,null,"Heat leak",-9,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-12","index":25,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-12"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","11HPa ~ 12HPa","12LPa ~ 11LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0]
["fraction","outlet","%",0,0]
["Flowrate",null,"g/s",225.06391648406338,66.563916484063398]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.355,1.1717734856507986]
["pressure","outlet","bar abs",19.344999999999999,1.1708187625208664]
["Operating","inlet","K",7.9237944138031366,5.3348967307537123]
["temperat.","outlet","K",6.9888849295174964,7.8310111137867011]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-997.68179797184371,1002.6997870154099,null,"","",""]
[null,null,null,null,null,null,"Heat leak",-5,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-13","index":26,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-13"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","12MPb ~ 13MPa","13LPd ~ 12LPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0.19330441195173353]
["fraction","outlet","%",100,0]
["Flowrate",null,"g/s",66.563916484063398,66.563916484063398]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",3.0100000000000002,1.1727282087807311]
["pressure","outlet","bar abs",3,1.1717734856507986]
["Operating","inlet","K",5.4348734949182358,4.3831043620451169]
["temperat.","outlet","K",4.4850000000000136,5.3348967307537123]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-493.64148802194546,498.64148802194518,null,"","",""]
[null,null,null,null,null,null,"Heat leak",-5,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]

{"sheet":"DS-HX-VLP","index":27,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[[13,0,14,0]]}
[]
[null,null,null,null,"Job nbr :","XXX",null,"Document number"]
[null,null,null,null,"Name :","ZZZZ"]
[null,null,null,null,null,null,null,"XXX-DS-YYY"]
["PROCESS",null,null,null,null,null,null,"Reference"]
["DATA",null,"PLATE-FIN HEAT EXCHANGER",null,null,null,null,"HX-VLP"]
[null,null,null,null,null,null,null,"Exch_Spec_HX-01.xls"]
[]
[null,"Type :","Horizontal/Vertical Aluminum brazed PFHE"]
[]
[null,null,null,null,null,null,"Run : ","ST!SC_MML__HX-VLP"]
["OPERATING CONDITIONS"]
["Fluid",null,"Units","HPa ~ HPb","VLPa ~ 0VLPa"]
["Nozzle name","in "]
[null,"out "]
["Fluid components",null,"molar %"]
[null,"Helium",null,100,100]
[]
[]
[]
["Liquid","inlet","%",0,0]
["fraction","outlet","%",0,0]
["Flowrate",null,"g/s",145.67443568338243,149.1]
["Maximum flowrate",null,"g/s"]
["Operating","inlet","bar abs",19.740000000000002,0.48599999999999993]
["pressure","outlet","bar abs",19.64,0.43599999999999994]
["Operating","inlet","K",300,18.103381794872718]
["temperat.","outlet","K",23.938158452081126,290]
["Pressure","expected","mbar"]
["drop","guaranteed","mbar"]
["Duty",null,"W",-210553.6784786355,210574.67993043977,null,"","",""]
[null,null,null,null,null,null,"Heat leak",-21,"W"]
["Design pressure",null,"bar g"]
["Design temperature",null,"°C"]
[]
["CORES CHARACTERISTICS"]
["Exchange","type "]
["fins","ht x thick ","mm x mm"]
[null,"density","FPI"]
["Distribution","type"]
["fins","ht x thick","mm x mm"]
[null,"density","FPI"]
["Distributors","inlet","mm"]
["length","outlet","mm"]
["Number of layers"]
["Effective width",null,"m"]
["Effective length",null,"m"]
["Headers","inlet","ND"]
["ND","outlet","ND"]
["Nozzles","inlet","ND"]
["ND","outlet","ND"]
["Manifolds","inlet"]
["ND","outlet"]
["Cores number",null,null,null,"Thickness","Parting sheets :",null,null,"mm"]
["Cores dimensions",null,"Width",null,null,"Side sheets :",null,null,"mm"]
["m",null,"Length",null,"Stacking Arrangement :"]
[null,null,"Height"]
[]
["Notes :"]
[]
[]
[]
[]
["Revision","DATE","BY",null,"VISA","CHECKED",null,"VISA","Page"]
[]
[]
[]
[null," ",null,null," "," "," "," "]